# Central cooling station with integrated refrigeration unit for 2 dispensers –

# ZKS-UKI 2

**Dimensions**

Length: 2,490 mm

Width: 600 mm

Height: 930 mm

###### Application

The central cooling station is used as a docking station with convection cooling for a maximum of 2 ZKS dispensers (UNI 60/60 ZKS or UNI 88/60 ZKS, each compatible to the central cooling station).

The universal dispenser is used to pre-cool system dishes and keep them cold, as well as to keep pre-portioned food cold.

The refrigeration unit is integrated in the central cooling station.

###### Model

**Design**

The central cooling station is designed as a fixed-position floor unit and stands on eight feet made of AISI 304, which can be adjusted to compensate for uneven floors.

The cooling station is permanently anchored to the floor with one fixing disk for each foot. The fixing disks are included in the scope of delivery.

The unit body is made of AISI 304 and is resistant to bending and twisting. The surface is micro-polished. The body is double-walled and insulated with polyurethane (PU) foam panels.

Docking centring devices ensure optimum docking of the dispensers on the central cooling station.

One all-round sealing frame each is located in the docking areas of the body to minimise cold loss when the dispenser is docked. For easier, safer locking of the dispensers, the central cooling station is equipped with one electromagnetic shear lock per docking point in the bottom area. Push-in synthetic profiles in the body ensure thermal separation of the exterior and interior body. These are used to avoid cold loss and the formation of condensation water.

The refrigeration unit of the ZKS-UKI is located in the housing body on the left next to the docking area.

The power connection cable with a Schuko plug is guided out of the unit at the bottom.

##### Active convection cooling

Cooling is activated with the On/Off switch integrated in the digital control.

Two air intake openings are located at the top and two air exhaust openings at the bottom in the body. If a docking area is not occupied with a dispenser, the respective air openings are closed with self-closing stainless-steel flaps.

When it is docked correctly, the electromagnetic shear lock locks the dispenser in place and connects it securely to the central cooling station. An integrated contact switch activates the convection cooling. The cold air is blown into the dispensers by a convection fan via the lower air exhaust openings and guided back out of the dispensers and into the central cooling station through the upper air intake openings. The air guidance ensures optimum circulation of the cold air in the dispenser. The refrigeration unit switches on automatically as necessary.

To separate the dispenser from the central cooling station, the electromagnetic shear lock is deactivated by the operating personnel by pressing a button. The dispenser can then be removed. Removing a ZK dispenser from the central cooling station causes cooling to be switched off immediately.

The interior temperature of the ZK dispensers can be regulated down to the degree from +4°C to +12°C with one digital regulator per dispenser.

The condensation-water catch trays are each located in an easily-accessible position next to the magnetic shear lock.

**Accessories/Options**

* Wall-mounted model

##### Technical data

Material: AISI 304

 Material No. 1.4301

 (AISI 304)

Insulating material: Polyurethane (PU)

Weight: approx. 160 kg

Capacity: Max. 2 ZKS dispensers

Refrigerant: R 134a

Temperature range: Adjustable down to the degree

 from +4°C to +12°C, at an ambient temperature of +32°C

Connected load: 220-240 V AC/ 50 Hz/ 0.8 kW

Emissions: The workplace-specific noise level of the unit is less than
 70 dB(A)

**Special features**

* Active convection cooling
* With integrated refrigeration unit
* Thermal separation
* Electromagnetic shear lock for easy, safe locking of dispensers
* Protection type IP X5

**Make**

Manufacturer: B.PRO

Model: ZKS-UKI 2

Order No. 372695