# Stainless steel SW 10x6 panelling set

**Application**

The panelling sets for B.PRO serving trolleys can be used anywhere a privacy shield is desired. The closed walls also prevent utensils in the serving trolley from accidentally falling out.

**Model**

The panelling set is made completely of stainless steel, AISI 304. It consists of two side walls and one rear wall. The panelling sections are folded over and have an edge at the top on the inside with which the panelling can be clamped behind the roller-burnished edge of the upper serving trolley shelf without using tools. With the aid of a second edge on the underside, these are securely fastened on the profile edge of the bottom serving trolley shelf. There are two ergonomic handle cut-outs each at the top of the side walls and the rear wall. These can be used to simply and safely hook in the panelling sections on the serving trolley. The panelling sections are completely removable for cleaning.

**Technical data**

Material: Stainless steel,

 AISI 304

Material thickness: 1.25 mm

Weight: 15,4 kg

For B.PRO serving trolleys: SW 10x6-2

 SW 10x6-3

 SW 10x6-2 BASIC

 SW 10x6-3 BASIC

### Special features

* For hooking in on B.PRO serving trolleys
* Completely removable for cleaning

**Make**

Manufacturer: B.PRO

Type: Stainless steel SW 10x6
panelling set

Order No. 375451