# Coloured SW 8x5 panelling set

**Application**

The panelling sets for B.PRO serving trolleys can be used anywhere a privacy shield is desired. The closed walls also prevent utensils in the serving trolley from accidentally falling out.

**Model**

The panelling set is made completely of powder-coated thin sheet galvanised on both sides. It consists of two side walls and one rear wall. The panelling sections are folded over and have an edge at the top on the inside with which the panelling can be clamped behind the roller-burnished edge of the upper serving trolley shelf without using tools. With the aid of a second edge on the underside, these are securely fastened on the profile edge of the bottom serving trolley shelf. There are two ergonomic handle cut-outs each at the top of the side walls and the rear wall. These can be used to simply and safely hook in the panelling sections on the serving trolley. The panelling sections are completely removable for cleaning.

**Technical data**

Material: Thin sheet, galvanised double-sided, powder-coated

Material thickness: 1.25 mm

Weight: 11,4 kg

Panelling colours: signal white, RAL 9003

 pearl white, RAL 1013

 pale brown, RAL 8025

 stone grey, RAL 7030

 umbra grey, RAL 7022

 graphite black, RAL 9011

 broom yellow, RAL 1032

 carmine red, RAL 3002

 sapphire blue, RAL 5003

 raspberry, Pantone 228 C

 lime, Pantone 382 C

 espresso, Pantone 4695 C

 apple green, Pantone 370 C

For B.PRO serving trolleys: SW 8X5-2

 SW 8x5-3

### Special features

* For hooking in on B.PRO serving trolleys
* Completely removable for cleaning

**Make**

Manufacturer: B.PRO

Type: Coloured SW 8x5 panelling set

Order No. 375453