# Coloured SW 10x6 panelling set + doors

**Application**

The panelling sets for B.PRO serving trolleys can be used anywhere a privacy shield is desired. The closed walls also prevent utensils in the serving trolley from accidentally falling out.

**Model**

The panelling set is made completely of powder-coated thin sheet galvanised on both sides. It consists of two side walls, one rear wall and two hinged doors at the front. The panelling sections are folded over and have an edge at the top on the inside with which the panelling can be clamped behind the roller-burnished edge of the upper serving trolley shelf without using tools. With the aid of a second edge on the underside, these are securely fastened on the profile edge of the bottom serving trolley shelf. There are two ergonomic handle cut-outs each at the top of the side walls and the rear wall. These can be used to simply and safely hook in the panelling sections on the serving trolley. The panelling sections are completely removable for cleaning. The hinged doors are fastened on the front on the round pipe clamps of the serving trolley using sturdy hinge parts made of glass-fibre reinforced synthetic. The doors can be opened by 270° and can be locked within the bumper rail. Fixing is carried out with magnets mounted in corresponding cut-outs in the side panelling. The closed doors are locked with an additional magnet, which is mounted at the centre front on the inside of the top and bottom serving trolley shelves.

**Technical data**

Material: Thin sheet, galvanised double-sided, powder-coated, glass-fibre reinforced PA 6.6

Material thickness: 1.25 mm

Weight: 23 kg

Panelling colours: Merlot red 19-1531 TPG

Sea blue 19-4234 TPG

Petrol green 18-5112 TPG

Candy red 17-1562 TPG

Neomint 15-5718 TPG

Signal white RAL 9003

Stone grey RAL 7030

Graphite black RAL 9011

Broom yellow RAL 1032

Traffic grey B RAL 7043

Lime Pantone 382 C

Apple green Pantone 370 C

For B.PRO serving trolleys: SW 10x6-2

 SW 10x6-3

 SW 10x6-2 BASIC

 SW 10x6-3 BASIC

(Doors not possible in combination with gusset plates!)

### Special features

* For simple mounting on B.PRO serving trolleys
* Side and rear wall completely removable for cleaning

**Make**

Manufacturer: B.PRO

Type: Coloured panelling set + doors

 SW 10x6

Order No. 375456