**BASIC LINE E-V – Roll-in counter, variable**

**Dimensions:**

Width: 550-2000 mm

*The final module equipment depends on the selected configuration or the selected equipment variant: Smart, Emotion or Design.*

**Basic module:**

Sturdy sheet metal structure. It can only be installed between two modules (suspended between modules).

Module length freely selectable between 550–2000 mm (roll-in niche)

**Top surface:**

The roll-in counter is equipped with a 40 mm high top surface of micro-polished stainless steel with smooth bevelling on all sides.

**Underframe:**

The side faces and the trim panel on the operator side are made of powder-coated thin sheet electrolytically galvanised on both sides: The standard colour of the basic buffet below the stainless-steel top surface:

Traffic grey B (RAL 7043)

*The following colours are available for the underframe as an alternative:* See under Customer-side front panelling B.PRO colour options. \*

**Customer-side front panelling:**

Customer-side front panelling

* made of thin sheet, electrolytically galvanised on both sides, powder-coated in B.PRO BASIC LINE colours. \*
* or particle board, coated with Resopal laminated sheet
* B.PRO colours: \*

merlot red 19-1531 TPG

sea blue 19-4234 TPG

petrol green 18-5112 TPG

candy red 17-1562 TPG

neomint 15-5718 TPG

signal white, RAL 9003

stone grey, RAL 7030

traffic grey B, RAL 7043

graphite black, RAL 9011

broom yellow, RAL 1032

lime, Pantone 382 C

apple green, Pantone 370 C

* Resopal laminated sheet in over 180 "Colours" or "Woods" Resopal decors

**Accessories/options:**

* Body colour: Side faces & panels, powder-coated in B.PRO colours. \*
* Tray slide made of stainless-steel round tube (tube 25 mm in diameter) on customer side and/or operator side, fold-down. At height of 885 mm or at reduced height of 785 mm for children's catering.
* Tray slide made of stainless-steel sheet on customer side and/or operator side, fold-down. At height of 885 mm or at reduced height of 785 mm for children's catering.
* Tray slide made of Multiplex panel, faced with Resopal on customer side and/or operator side, fold-down. At height of 885 mm or at reduced height of 785 mm for children's catering.
* Plate slide made of stainless-steel sheet on customer side and/or operator side, fold-down. Flush with the top surface at height of
900 mm.
* Plate slide made of Multiplex panel, faced with Resopal on customer side and/or operator side, fold-down. Flush with the top surface at height of 900 mm.
* Stainless-steel skirting panels on customer side

**Technical data:**

Material: Stainless steel (AISI 304) micro-polished; combined with powder-coated thin sheet electrolytically galvanised on both sides.

Weight: ---

*The module's weight depends on the module width or on the optional accessories.*

**Special features:**

* Module length freely selectable between
550-2200 mm
* Micro-polished surface made of stainless steel
* Fold-down tray and plate slides made of stainless-steel round tube, stainless-steel sheet and Multiplex with Resopal lining.
* Large selection of colour scheme and customisation options

**Make:**

Manufacturer: B.PRO

Model: BASIC LINE E-V

Order No.: 381 886