**BASIC LINE IE-V – Inside corner, variable**

**Dimensions:**

Width: Depends on the angle

Depth: 690 mm

Depth 1: 775 mm

(= with folded-down tray slide on customer side)

Depth 2: 990 mm

(= with folded-up tray slide on customer side)

Height of top surface: 900 mm

*The final module equipment depends on the selected configuration or the selected equipment variant: Smart, Emotion or Design.*

**Basic module:**

Mobile module, based on a sturdy, self-supporting sheet metal structure.

Angle variable, freely selectable between 45° and 90°.

**Top surface:**

The corner module is equipped with a 40 mm high top surface of micro-polished stainless steel with smooth bevelling on all sides.

**Underframe:**

The side faces and the trim panel on the operator side are made of powder-coated thin sheet electrolytically galvanised on both sides: The standard colour of the basic buffet below the stainless-steel top surface:

Traffic grey B (RAL 7043)

*The following colours are available for the underframe as an alternative:* See under Customer-side front panelling B.PRO colour options. \*

The castors are mounted on the lower surface of the side faces: 2 twin steering castors with brakes on the operator side, 2 twin steering castors on the customer side, castor diameter: 75 mm.

**Customer-side front panelling:**

Customer-side front panelling

* made of thin sheet, electrolytically galvanised on both sides, powder-coated in B.PRO BASIC LINE colours. \*
* or particle board, coated with Resopal laminated sheet
* B.PRO colours: \*

signal white, RAL 9003

pearl white, RAL 1013

pale brown, RAL 8025

stone grey, RAL 7030

umbra grey, RAL 7022

traffic grey B, RAL 7043

graphite black, RAL 9011

broom yellow, RAL 1032

carmine red, RAL 3002

sapphire blue, RAL 5003

raspberry, Pantone 228 C

lime, Pantone 382 C

espresso, Pantone 4695 C

apple green, Pantone 370 C

* Resopal laminated sheet in over 180 "Colours" or "Woods" Resopal decors

**Accessories/options:**

* Body colour: Side faces & panels, powder-coated in B.PRO colours. \*
* Tray slide made of stainless-steel round tube (tube 25 mm in diameter) on customer side and/or operator side, fold-down. At height of 885 mm or at reduced height of 785 mm for children's catering.
* Tray slide made of stainless-steel sheet on customer side and/or operator side, fold-down. At height of 885 mm or at reduced height of 785 mm for children's catering.
* Tray slide made of Multiplex panel, faced with Resopal on customer side and/or operator side, fold-down. At height of 885 mm or at reduced height of 785 mm for children's catering.
* Plate slide made of stainless-steel sheet on customer side and/or operator side, fold-down. Flush with the top surface at height of   
  900 mm.
* Plate slide made of Multiplex panel, faced with Resopal on customer side and/or operator side, fold-down. Flush with the top surface at height of 900 mm.
* Module connection set to permanently interconnect two buffets, including profile panel to cover the gap between two modules.
* Stainless-steel castors, 125 mm in diameter,   
  4 steering castors, 2 of which have brakes. Total height is increased by 60 mm, underframe height is then 960 mm
* Adjustable feet made of stainless steel (instead of castors)
* Stainless-steel skirting panels on customer side/short side right/left (can only be ordered in conjunction with adjustable feet)

**Technical data:**

Material: Stainless steel (AISI 304) micro-polished; combined with powder-coated thin sheet electrolytically galvanised on both sides.

Weight: ---

*The module's weight depends on the angle or on the optional accessories.*

**Special features:**

* Angle variable, freely selectable between   
  45° and 90°.
* Micro-polished surface made of stainless steel
* Fold-down tray and plate slides made of stainless-steel round tube, stainless-steel sheet and Multiplex with Resopal lining.
* Large selection of colour scheme and customisation options

**Make:**

Manufacturer: B.PRO

Model: BASIC LINE IE-V

Order No.: 381 888