**BASIC LINE K-4 - Cash register booth**

**Dimensions:**

Width: 1595 mm

Depth: 690 mm

Depth 1: 775 mm

(= with folded-down tray slide on customer side)

Depth 2: 990 mm

(= with folded-up tray slide on customer side)

Height of top surface: 900 mm

*The final module equipment depends on the selected configuration or the selected equipment variant: Smart, Emotion or Design.*

**Basic module:**

Mobile module, based on a sturdy, self-supporting sheet metal structure, installed ready to plug in, with approx. 2 m connection cable and plug.

Cash register table can be positioned on left or right on operator side.

**Top surface:**

The cash register module is equipped with a 40 mm high top surface of micro-polished stainless steel with smooth bevelling on all sides. With stainless-steel table top with opening for cable routing. With drawer beneath stainless-steel table top.

**Underframe:**

The side faces and the trim panel on the operator side are made of powder-coated thin sheet electrolytically galvanised on both sides: The standard colour of the basic buffet below the stainless-steel top surface:

Traffic grey B (RAL 7043)

*The following colours are available for the underframe as an alternative:* See under Customer-side front panelling B.PRO colour options. \*

Two additional socket outlets with 230 V Schuko socket each, installed on operator side on inside beneath table top. The maximum permitted power input for socket outlets to connect external units depends on the unit equipment.

In the foot space beneath the table top with footrest installed at an angle

The castors are mounted on the lower surface of the side faces: 2 twin steering castors with brakes on the operator side, 2 twin steering castors on the customer side, castor diameter: 75 mm.

**Customer-side front panelling:**

Customer-side front panelling

* made of thin sheet, electrolytically galvanised on both sides, powder-coated in B.PRO BASIC LINE colours. \*
* or particle board, coated with Resopal laminated sheet
* B.PRO colours: \*

merlot red 19-1531 TPG

sea blue 19-4234 TPG

petrol green 18-5112 TPG

candy red 17-1562 TPG

neomint 15-5718 TPG

signal white, RAL 9003

stone grey, RAL 7030

traffic grey B, RAL 7043

graphite black, RAL 9011

broom yellow, RAL 1032

lime, Pantone 382 C

apple green, Pantone 370 C

* Resopal laminated sheet in over 180 "Colours" or "Woods" Resopal decors

**Accessories/options:**

* Body colour: Side faces & panels, powder-coated in B.PRO colours. \*
* Tray slide made of stainless-steel round tube (tube 25 mm in diameter) on customer side and/or operator side, fold-down. At height of 885 mm or at reduced height of 785 mm for children's catering.
* Tray slide made of stainless-steel sheet on customer side and/or operator side, fold-down. At height of 885 mm or at reduced height of 785 mm for children's catering.
* Tray slide made of Multiplex panel, faced with Resopal on customer side and/or operator side, fold-down. At height of 885 mm or at reduced height of 785 mm for children's catering.
* Plate slide made of stainless-steel sheet on customer side and/or operator side, fold-down. Flush with the top surface at height of   
  900 mm.
* Plate slide made of Multiplex panel, faced with Resopal on customer side and/or operator side, fold-down. Flush with the top surface at height of 900 mm.
* Shelf made of stainless-steel round tube (tube 25 mm in diameter) on short side, right and/or left, fold-down. At height of 885 mm or at reduced height of 785 mm for children's catering.
* Shelf made of stainless-steel sheet on short side, right and/or left, fold-down. Flush with the top surface (900 mm) or at height of   
  885 mm or reduced height of 785 mm for children's catering.
* Shelf made of Multiplex panel, faced with Resopal on short side, right and/or left, fold-down. Flush with the top surface (900 mm) or at height of 885 mm or reduced height of   
  785 mm for children's catering.
* Mains connection with 16A CEE plug, 400 V
* Module connection set to permanently interconnect two buffets, including profile panel to cover the gap between two modules.
* Stainless-steel castors, 125 mm in diameter,   
  4 steering castors, 2 of which have brakes. Total height is increased by 60 mm, underframe height is then 960 mm
* Adjustable feet made of stainless steel (instead of castors)
* Stainless-steel skirting panels on customer side/short side right/left (can only be ordered in conjunction with adjustable feet)

**Technical data:**

Material: Stainless steel (AISI 304) micro-polished; combined with powder-coated thin sheet electrolytically galvanised on both sides.

Weight: approx. 95 kg (without options)

Connected load: 230 V/16 A/1N PE/

50–60 Hz

*The module's connected load depends on the optional accessories.*

**Special features:**

* Cash register table design optionally on left or right, with opening for cable routing
* 2 socket outlets with 230 V Schuko socket each
* Footrest
* Micro-polished surface made of stainless steel
* Fold-down tray and plate slides made of stainless-steel round tube, stainless-steel sheet and Multiplex with Resopal lining.
* Large selection of colour scheme and customisation options

**Make:**

Manufacturer: B.PRO

Model: BASIC LINE K-4

Order No.: 381 890