**BASIC LINE AKV-3 – Attached showcase, refrigerated, similar to 3 x GN 1/1**

**Dimensions:**

Width: 1255 mm

Depth: 690 mm

Depth 1: 775 mm

(= with folded-down tray slide on customer side)

Depth 2: 990 mm

(= with folded-up tray slide on customer side)

Height of top surface: 900 mm

Height, including attached showcase: 1400 mm

*The final module equipment depends on the selected configuration or the selected equipment variant: Smart, Emotion or Design.*

**Basic module:**

Mobile module, based on a sturdy, self-supporting sheet metal structure, installed ready to plug in, with approx. 2 m connection cable and plug.

**Top-mounted unit:**

A convection-cooled attached showcase (make: IDEAL AKE) with 2 levels made of stainless steel (chrome nickel steel) is permanently positioned on the 40 mm high, micro-polished stainless-steel top surface with smooth bevelling on all sides. There is an extensive, coated finned evaporator with convection beneath the showcase unit cover. The showcase features 6 customer-side serving doors and 2 operator-side sliding doors made of insulated glass. The side glazing panes are also made of insulated glass. The height-adjustable middle shelf is made of toughened safety glass. The interior lighting is horizontal and protected beneath the unit cover. There is an electronic temperature control with digital temperature display, an on/off switch and a switch for lighting above the sliding doors on the operator side. Continuous speed control for the fans. Temperature range: +6 °C to +12 °C at +25 °C ambient temperature and 60% relative humidity.

**Underframe:**

The side faces and the trim panels on the customer and operator sides are made of powder-coated thin sheet electrolytically galvanised on both sides. The forced-air cooled refrigeration unit is installed, ready to plug, in the underframe on the operator side. With fully automatic air defrosting and a removable condensation water tray.

The standard colour of the basic buffet below the stainless-steel top surface:

Traffic grey B (RAL 7043)

*The following colours are available for the underframe as an alternative:* See under Accessories/B.PRO colour options. \*

Two additional socket outlets with a 230 V Schuko socket each (one to connect the showcase) are installed on the side face interior on the operator side.

The castors are mounted on the lower surface of the side faces: 2 twin steering castors with brakes on the operator side, 2 twin steering castors on the customer side, castor diameter: 75 mm.

**Customer-side front panelling:**

Customer-side front panelling

* made of thin sheet, electrolytically galvanised on both sides, powder-coated in B.PRO BASIC LINE colours. \*
* or particle board, coated with Resopal laminated sheet
* B.PRO colours: \*

signal white, RAL 9003

pearl white, RAL 1013

pale brown, RAL 8025

stone grey, RAL 7030

umbra grey, RAL 7022

traffic grey B, RAL 7043

graphite black, RAL 9011

broom yellow, RAL 1032

carmine red, RAL 3002

sapphire blue, RAL 5003

raspberry, Pantone 228 C

lime, Pantone 382 C

espresso, Pantone 4695 C

apple green, Pantone 370 C

* Resopal laminated sheet in over 180 "Colours" or "Woods" Resopal decors

**Accessories/options:**

* Body colour: Side faces & panels, powder-coated in B.PRO colours. \*
* Attached showcase with 3 levels instead of 2. With 9 serving doors on the customer side and 2 height-adjustable middle shelves made of toughened safety glass; total unit height 1600 mm.
* Tray slide made of stainless-steel round tube (tube 25 mm in diameter) on customer side and/or operator side, fold-down. At height of 885 mm or at reduced height of 785 mm for children's catering.
* Tray slide made of stainless-steel sheet on customer side and/or operator side, fold-down. At height of 885 mm or at reduced height of 785 mm for children's catering.
* Tray slide made of Multiplex panel, faced with Resopal on customer side and/or operator side, fold-down. At height of 885 mm or at reduced height of 785 mm for children's catering.
* Plate slide made of stainless-steel sheet on customer side and/or operator side, fold-down. Flush with the top surface at height of   
  900 mm.
* Plate slide made of Multiplex panel, faced with Resopal on customer side and/or operator side, fold-down. Flush with the top surface at height of 900 mm.
* Shelf made of stainless-steel round tube (tube 25 mm in diameter) on short side, right and/or left, fold-down. At height of 885 mm or at reduced height of 785 mm for children's catering.
* Shelf made of stainless-steel sheet on short side, right and/or left, fold-down. Flush with the top surface (900 mm) or at height of   
  885 mm or reduced height of 785 mm for children's catering.
* Shelf made of Multiplex panel, faced with Resopal on short side, right and/or left, fold-down. Flush with the top surface (900 mm) or at height of 885 mm or reduced height of 785 mm for children's catering.
* Mains connection with 16A CEE plug, 400 V
* Power supply 220 V/60 Hz instead of 230 V/50 Hz.
* Stainless-steel base bottom, to hold B.PROTHERM BPT 420 K / KBUH / KBRUH, for example
* Module connection set to permanently interconnect two buffets, including profile panel to cover the gap between two modules.
* Stainless-steel castors, 125 mm in diameter,   
  4 steering castors, 2 of which have brakes. Total height is increased by 60 mm, underframe height is then 960 mm
* Adjustable feet made of stainless steel (instead of castors)
* Stainless-steel skirting panels on customer side/short side right/left (can only be ordered in conjunction with adjustable feet)

**Technical data:**

Material: Stainless steel (AISI 304) micro-polished; combined with powder-coated thin sheet electrolytically galvanised on both sides.

Weight: approx. 175 kg (without options)

Temperature range: +6 °C to +12 °C at +25 °C ambient temperature and 60% relative humidity.

Refrigerant: R-134a

Connected load: 230 V/16 A/1N PE/50 Hz

Emissions: The workplace-specific

noise level of the unit is

less than 70 dB(A)

*The module's connected load depends on the optional accessories.*

**Special features:**

* Electronic temperature control with digital temperature display
* Whisper-quiet, energy-saving refrigeration unit
* Micro-polished surface made of stainless steel
* Fold-down tray and plate slides made of stainless-steel round tube, stainless-steel sheet and Multiplex with Resopal lining.
* Large selection of colour scheme and customisation options

**Make:**

Manufacturer: B.PRO

Model: BASIC LINE AKV-3

Order No.: 381 893