**BASIC LINE UK-3 Kids – Cold buffet with active convection cooling 3 x GN 1/1 with low module height for children's catering**

**Dimensions:**

Width: 1255 mm

Depth: 690 mm

Depth 1: 775 mm

(= with folded-down tray slide on customer side)

Depth 2: 990 mm

(= with folded-up tray slide on customer side)

Height of top surface: 750 mm

Height, including bridge attachment: 1155 mm

*The final module equipment depends on the selected configuration.*

**Basic module:**

Mobile module, based on a sturdy, self-supporting sheet metal structure, installed ready to plug in, with approx. 2 m connection cable and plug.

**Top surface:**

The convection-cooled tray with CFC-free insulation is seamlessly welded into the 40 mm high, micro-polished stainless-steel top surface with smooth bevelling on all sides. The cooling tray is designed to hold three 1/1-GN-200 containers or their subdivisions. The stainless-steel inner section of the cooling tray can be completely removed for cleaning. The large-area finned evaporator with fan is located beneath. The finned evaporator can be folded up with a locking bar and locked in place during cleaning and service work. The lower tray bottom is stamped with a downhill slope toward the centre of the tray. The condensation water drains off into a manually emptied condensation-water catch tray.

The on/off switch for the refrigeration unit, the electronic cooling point control with digital design and the optional LED lighting are installed in the operator-side recessed panel on refrigeration unit compartment to protect it against impact.

**Underframe:**

The side faces and the trim panel in front of the well section on the customer and operator sides are made of powder-coated thin sheet electrolytically galvanised on both sides. The installation compartment for the fully hermetically enclosed refrigeration unit is made of the same material. The refrigeration unit is conveniently accessible from the operator side for cleaning and servicing by unscrewing the installation compartment cover. The standard colour of the basic buffet below the stainless-steel top surface:

Traffic grey B (RAL 7043)

*The following colours are available for the underframe as an alternative:* See under Accessories/B.PRO colour options. \*

The castors are mounted on the lower surface of the side faces: 2 twin steering castors with brakes on the operator side, 2 twin steering castors on the customer side, castor diameter: 75 mm.

**Accessories/options:**

* Body colour: Side faces & panels, powder-coated in B.PRO colours. \*
* Front panelling on customer side, between side faces, easy to remove and mount,
* made of thin sheet, electrolytically galvanised on both sides, powder-coated in B.PRO BASIC LINE colours. \*
* or particle board, coated with Resopal laminated sheet
* Operator-side front panelling, featured as hinged doors between the side faces.
* Made of thin sheet, electrolytically galvanised on both sides, powder-coated in B.PRO BASIC LINE colours \* or faced with Resopal laminated sheet.
* B.PRO colours: \*

signal white, RAL 9003

pearl white, RAL 1013

pale brown, RAL 8025

stone grey, RAL 7030

umbra grey, RAL 7022

traffic grey B, RAL 7043

graphite black, RAL 9011

broom yellow, RAL 1032

carmine red, RAL 3002

sapphire blue, RAL 5003

raspberry, Pantone 228 C

lime, Pantone 382 C

espresso, Pantone 4695 C

apple green, Pantone 370 C

* Resopal laminated sheet in over 180 "Colours" or "Woods" Resopal decors
* Standard bridge attachment with sneeze guard.

The smooth-surfaced, fully panelled bridge attachment of micro-polished stainless-steel sheet is mounted in the centre of the top surface. Stainless-steel brackets for fastening the sneeze guard glass are mounted on the left and right of the bridge attachment. The brackets are U-shaped to protect the glass against damage on the short sides. Made of toughened safety glass, the sneeze guard is mounted, so it slopes towards the customer side and provides a pass-through opening. Pass-through height: 280 mm.

* Highline bridge attachment with toughened safety glass sneeze guard is attached, so that it is horizontal to the top surface on the customer side and provides a pass-through opening. Pass-through height: 395 mm.
* Operator-side sneeze guard made of toughened safety glass.

Pass-through height standard attachment:
280 mm

Pass-through height Highline attachment:
395 mm

* Customer-side sneeze guard made of toughened safety glass, without pass-through, down to the top surface.
* LED lighting with 3 LED spotlights is installed in the bridge attachment. Spotlights can be switched off and on separately.
* Tray slide made of stainless-steel round tube (tube 25 mm in diameter) on customer side and/or operator side, fold-down. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Tray slide made of stainless-steel sheet on customer side and/or operator side, fold-down. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Tray slide made of Multiplex panel, faced with Resopal on customer side and/or operator side, fold-down. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Plate slide made of stainless-steel sheet on customer side and/or operator side, fold-down. Flush with the top surface at height of 750mm. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Plate slide made of Multiplex panel, faced with Resopal on customer side and/or operator side, fold-down. Flush with the top surface at height of 750mm. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Shelf made of stainless-steel round tube (tube 25 mm in diameter) on short side, right and/or left, fold-down. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Shelf made of stainless-steel sheet on short side, right and/or left, fold-down. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Shelf made of Multiplex panel, faced with Resopal on short side, right and/or left, fold-down. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Switch panel cover top surface. To cover switches and operating elements
* Additional socket outlets. Two additional socket outlets with 230 V Schuko socket each on operator side, installed in the refrigeration unit interior in the right-hand side face. The maximum permitted power input for socket outlets to connect external units depends on the unit equipment.
* Mains connection with 16A CEE plug, 400 V
* Power supply 220 V/60 Hz instead of 230 V/50 Hz.
* Module connection set to permanently interconnect two buffets, including profile panel to cover the gap between two modules.
* Stainless-steel castors, 125 mm in diameter,
4 steering castors, 2 of which have brakes. Total height is increased by 60 mm, underframe height is then 810 mm
* Adjustable feet made of stainless steel (instead of castors)
* Stainless-steel skirting panels on customer side/short side right/left (can only be ordered in conjunction with adjustable feet)
* Stainless-steel slatted shelf, 3 pieces for cooling bottled beverages
* Stainless-steel ventilation cover, two pieces, to cover the gap between cooling tray and stainless-steel top surface

**Technical data:**

Material: Stainless steel (AISI 304) micro-polished; combined with powder-coated thin sheet electrolytically galvanised on both sides.

Weight: Depending on equipment

Capacity: max. 3 x GN 1/1-200

Temperature range: The temperature is factory pre-set to +7 °C and can be set to values between +2 °C and +15 °C\* when the ambient temperature is max. +32 °C

Refrigerant: R-134a

Connected load: 230 V/16 A/1N PE/50 Hz

Emissions: The workplace-specific

 noise level of the unit is

 less than 70 dB(A)

*The module's connected load depends on the optional accessories.*

\* The temperature is reached at the geometric centre of the cooling tray

**Special features:**

* Convection-cooling tray with fan and large-area finned evaporator
* Electronic cooling point control with digital display
* Whisper-quiet, energy-saving refrigeration unit
* Sneeze guard made of toughened safety glass
* Micro-polished surface made of stainless steel
* Two-section safety drain valve
* Fold-down tray and plate slides made of stainless-steel round tube, stainless-steel sheet and Multiplex with Resopal lining.
* Large selection of colour scheme and customisation options

**Make:**

Manufacturer: B.PRO

Model: BASIC LINE UK-3 Kids

Order No.: 381 901