**BASIC LINE N-3 Kids – Plain buffet, similar to 3 x GN 1/1 with low module height for children's catering**

**Dimensions:**

Width: 1255 mm

Depth: 690 mm

Depth 1: 775 mm

(= with folded-down tray slide on customer side)

Depth 2: 990 mm

(= with folded-up tray slide on customer side)

Height of top surface: 750 mm

Height, including bridge attachment: 1155 mm

*The final module equipment depends on the selected configuration.*

**Basic module:**

Mobile module, based on a sturdy, self-supporting sheet metal structure.

If electric options/components are configured, the module is installed ready to plug in, with approx. 2 m connection cable and plug.

**Top surface:**

The plain buffet is equipped with a 40 mm high top surface of micro-polished stainless steel with smooth bevelling on all sides. An approx. 240 mm high trim panel is located below the top surface on both long sides.

**Underframe:**

The side faces and the trim panel in front of the well section on the customer and operator sides are made of powder-coated thin sheet electrolytically galvanised on both sides. The standard colour of the basic buffet below the stainless-steel top surface:

Traffic grey B (RAL 7043)

*The following colours are available for the underframe as an alternative:* See under Accessories/B.PRO colour options. \*

The castors are mounted on the lower surface of the side faces: 2 twin steering castors with brakes on the operator side, 2 twin steering castors on the customer side, castor diameter: 75 mm.

**Accessories/options:**

* Body colour: Side faces & panels, powder-coated in B.PRO colours. \*
* Front panelling on customer side, between side faces, easy to remove and mount,
* made of thin sheet, electrolytically galvanised on both sides, powder-coated in B.PRO BASIC LINE colours. \*
* or particle board, coated with Resopal laminated sheet
* Operator-side front panelling, featured as hinged doors between the side faces.
* Made of thin sheet, electrolytically galvanised on both sides, powder-coated in B.PRO BASIC LINE colours \* or faced with Resopal laminated sheet.
* B.PRO colours: \*

merlot red 19-1531 TPG

sea blue 19-4234 TPG

petrol green 18-5112 TPG

candy red 17-1562 TPG

neomint 15-5718 TPG

signal white, RAL 9003

stone grey, RAL 7030

traffic grey B, RAL 7043

graphite black, RAL 9011

broom yellow, RAL 1032

lime, Pantone 382 C

apple green, Pantone 370 C

* Resopal laminated sheet in over 180 "Colours" or "Woods" Resopal decors
* Standard bridge attachment with sneeze guard.

The smooth-surfaced, fully panelled bridge attachment of micro-polished stainless-steel sheet is mounted in the centre of the top surface. Stainless-steel brackets for fastening the sneeze guard glass are mounted on the left and right of the bridge attachment. The brackets are U-shaped to protect the glass against damage on the short sides. Made of toughened safety glass, the sneeze guard is mounted, so it slopes towards the customer side and provides a pass-through opening. Pass-through height: 280 mm.

* Highline bridge attachment with toughened safety glass sneeze guard is attached, so that it is horizontal to the top surface on the customer side and provides a pass-through opening. Pass-through height: 395 mm.
* Operator-side sneeze guard made of toughened safety glass.

Pass-through height standard attachment:
280 mm

Pass-through height Highline attachment:
395 mm

* Customer-side sneeze guard made of toughened safety glass, without pass-through, down to the top surface.
* Three individually switchable ceramic radiators with a power consumption of 200 W each. Fitted into the bridge attachment. The ceramic radiators are protected against being touched directly with a close-meshed stainless-steel grid plate.
* LED lighting with 3 LED spotlights (or 4 LED spotlights when radiant heater/LED combination) are installed in the bridge attachment. Spotlights can be switched off and on separately from the radiant heaters. Light colour option between warm white
3000 K or neutral white 4000 K.
* Tray slide made of stainless-steel round tube (tube 25 mm in diameter) on customer side and/or operator side, fold-down. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Tray slide made of stainless-steel sheet on customer side and/or operator side, fold-down. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Tray slide made of Multiplex panel, faced with Resopal on customer side and/or operator side, fold-down. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Plate slide made of stainless-steel sheet on customer side and/or operator side, fold-down. Flush with the top surface at height of 750 mm. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Plate slide made of Multiplex panel, faced with Resopal on customer side and/or operator side, fold-down. Flush with the top surface at height of 750mm. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Shelf made of stainless-steel round tube (tube 25 mm in diameter) on short side, right and/or left, fold-down. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Shelf made of stainless-steel sheet on short side, right and/or left, fold-down. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Shelf made of Multiplex panel, faced with Resopal on short side, right and/or left, fold-down. With child-safe lock mechanism. Fixed locking thanks to locking pins.
* Switch panel cover top surface To cover switches and operating elements
* Additional socket outlets. Two additional socket outlets with 230 V Schuko socket each, on operator side installed on inside of right side face. The maximum permitted power input for socket outlets to connect external units depends on the unit equipment.
* Mains connection with 16A CEE plug, 400 V
* Base bottom made of stainless steel
* Module connection set to permanently interconnect two buffets, including profile panel to cover the gap between two modules.
* Stainless-steel castors, 125 mm in diameter,
4 steering castors, 2 of which have brakes. Total height is increased by 60 mm, underframe height is then 810 mm
* Adjustable feet made of stainless steel (instead of castors)
* Stainless-steel skirting panels on customer side/short side right/left (can only be ordered in conjunction with adjustable feet)

**Technical data:**

Material: Stainless steel (AISI 304) micro-polished; combined with powder-coated thin sheet electrolytically galvanised on both sides.

Weight: Depending on equipment

Capacity: same as 3 x GN 1/1

Connected load: ---

*The module's connected load depends on the optional accessories.*

**Special features:**

* Sneeze guard made of toughened safety glass
* Micro-polished surface made of stainless steel
* Fold-down tray and plate slides made of stainless-steel round tube, stainless-steel sheet and Multiplex with Resopal lining.
* Large selection of colour scheme and customisation options

**Make:**

Manufacturer: B.PRO

Model: BASIC LINE N-3 Kids

Order No.: 381 903