# B.PROTHERM BPT E 2 x 12 combi N/N Special



**Dimensions**

Length: 590 mm

Width: 821 mm

Height: 1532 mm

**Model**

**Design**

The B.PROTHERM is made of AISI 304 stainless steel. The surface is micro-polished.

Body and hinged doors are double-walled and fitted with CFC-free PUR foam panels for thermal insulation. As a combi model, the trolley features two separate, thermally insulated compartments on top of one another.

Two compartments a neutral design.

The B.PROTHERM is mobile thanks to corrosion-resistant synthetic castors as per DIN 18867, Part 8 (2 fixed and 2 steering castors with brakes, castor diameter 125 mm). The sturdy, synthetic base structure with integrated all-round bumper rail protects the unit and furniture from damage.

**Body**

The BPT E 2 x 12 combi N/N's enclosed top cover features stacking nubs, meaning B.PROTHERM synthetic containers can be stacked on it. The base and rear and side walls are fitted with all-round edge radius R2 and are spot-welded at their points of contact (hygienic type HS). The interior is fully equipped with 12 pairs of deep-drawn stainless steel ledge walls per compartment for easy cleaning and maximum hygiene. The support ledges have a uniform spacing of 38.3 mm to hold Gastronorm containers size GN 1/1 or their subdivisions. This means all common spacing dimensions (about 75 mm, 115 mm) can be housed in a single unit and ensures efficient use of the interior.

Interior and exterior body are vertically connected with synthetic profiles and thermally separated.

The B.PROTHERM is equipped with 4 vertical push handles as standard to ensure optimum handling on all sides. The ergonomic length of the handles makes the trolley easy to manoeuvre.

The push handles are located within the bumper rail to prevent the hands from being crushed when rolling through doors and narrow corridors. The helix cord and plug holder are attached on the unit rear and also within the all-round bumper rail.

The B.PRO control is integrated into the top of the unit, making it easy to use. It contains the unit on/off button, a menu button, a function button and an up/down button, e.g. to regulate the temperature in the interior precisely.

**Doors**

The trolley is equipped with two doors on its front that can be opened 270°. The doors are inside the bumper rail when open or closed and are thus protected from damage. The push handles are still accessible when the door is open. The robust door hinges are made of stainless steel investment casting. The hinge design eliminates risk of injury if a user should accidentally take hold of the hinge. A ventilation flap is fitted into the door on the convection-heated compartment to regulate moisture in the container interior.

The doors are also fitted with an all-round, food-safe seal (TPE) that closes against the trolley body and can be removed.

The doors are fitted with a 2-point locking system. It is easy to open from the outside by simply pushing up the door handle.

The B.PROTHERM has a push-button which glows in the dark in its interior. The patented panic opening can be identified if someone should get accidentally locked inside the interior and the door lock can be unlocked from the inside by pressing the button. What is known as the afterglow effect meets the requirements for safety-relevant components specified in ISO 16069.

**Options**

* Can be customised with powder coating on body and doors in 12 colours
* Digitisation/connectivity for digital hygiene, temperature and process management using optionally built-in sensor technology
* Additional socket on rear panel (instead of plug holder) for coupling additional units
* Top with stainless steel railing on 3 sides
* (Smooth) top with stainless steel railing on 4 sides
* Hygienic type H1
* Door, lockable
* Convenient door opening with foot operation
* Stainless-steel castors, 125 mm in diameter, 2 fixed and 2 steering castors with brakes
* Anti-static castors, 125 mm in diameter, 2 fixed and 2 steering castors with brakes, corrosion-resistant in compliance with DIN 18867-8, synthetic
* Galvanised steel castors, 160 mm in diameter,

2 fixed and 2 steering castors with brakes

* Galvanised steel castors with elastic tyres, 160 mm in diameter, 2 fixed and 2 steering castors with brakes
* Stainless-steel castors, 160 mm in diameter, 2 fixed and 2 steering castors with brakes
* Stainless-steel castors with elastic tyres, 160 mm in diameter, 2 fixed and 2 steering castors with brake

**Accessories**

* Thermal separation element for the neutral compartment to sub-divide the interior to allow use of different temperature zones.
* Eutectic plate -3 °C, synthetic

(Order no.: 568 136)

* Eutectic plate -12 °C, synthetic

(Order no.: 573 332)

* Slide-in frame to sub-divide GN containers

with max. depth 150 mm (order no. 564 352)

* GN support bars for variable insertion of GN containers of the size GN 1/4, GN 1/6, GN 1/9 in the slide-in frame (ST 3 order no. 550 650; ST 5 order no. 550 651)
* Menu card holder for the door on front, stainless steel, to attach DIN A5 and DIN A6 menu cards (order no. 575 230)
* BPT E menu card, DIN A6 (order no. 564 353)
* Special pen for marking BPT E menu cards (order no. 564 361)
* Menu card box, synthetic (order no. 564 355)

**Technical data**

Material: Stainless steel,

 synthetic

Insulating material: PUR foam panels, CFC-free

Weight: 92 kg

Capacity: 6 x GN 1/1-65 per compartment

 2 x 12 pairs of deep-drawn support ledges

 Space between ledges of 38.3 mm

Protection type: IPX5

**Special features**

* Two thermally separated compartments for different temperature ranges
* Extremely efficient, flexible use of interior thanks to uniform space between ledges of 38.3 mm
* Deep-drawn stainless steel ledge walls for easy cleaning and maximum hygiene.
* Sturdy, enclosed, solid, synthetic base structure with integrated all-round bumper rail.
* Hinged door with door opening of 270°, with lock
* Optional connectivity function

**Make**

Manufacturer: B.PRO

Model: BPT E 2 x 12 combi N/N

 B.PROTHERM

Order no. 386 615