# Double built-in glass-rinsing basin ED 7.1x5.8

**Dimensions:**

Exterior dimensions:

Length: 710 mm

Width: 580 mm

Basin size:

Length: 302mm

Width: 502 mm

Depth: 300 mm

Cut-out dimensions:

Length: 690 mm

Width: 560 mm

**Design:**

Basin and top surface deep-drawn. With securing elements and suitable all-around seal; for building into Resopal or AISI 304 table tops.

Basin surfaces fully brushed; basins without overflow indentation.

Drain: 1 ½" each.

**Accessories:**

* 2x 1 ½" tube overflow; Order no.: 223 063
* Drain connection for double basin

 Order No.: 369 969

**Technical data:**

Material: Stainless steel

Material no.: 1.4301

**Make:**

Manufacturer: B.PRO

Model: EE 7.1x5.8

Order No.: 505 037