# Serving trolley SW 8X5-2

**Dimensions**

Length: 900 mm

Width: 600 mm

Height: 950 mm

Inside dimensions:

Height between shelves: 585 mm

Shelves: 800 x 500 mm

**Design**

The serving trolley is made of stainless steel, AISI 304. There are two welded-in, deep-drawn shelves between a sturdy round tube 25 mm in diameter. The shelf surfaces are micro-polished. The round tubes on the short sides are used as push handles. A 35-mm turned-down, all-round profile edge on the shelves, the roller-burnished shelf rim and single-piece welded seams between the tube frame and shelves all make the serving trolley sturdier.

A noise-insulating anti-drumming mat is positioned beneath the shelves.

The serving trolley is mobile on galvanised steel castors (4 steering castors, 2 of which have brakes, castor diameter 125 mm). The castors are inserted into the tube frame. Synthetic (polyethylene) wall guards at all four corners protect against damage.

**Accessories/options**

* Stainless-steel waste container AFB 4 x 2 x 2.5, with hanging device, 18.5 litres (Order No.: 555 509)
* Stainless-steel cutlery holder BGN 1/3-150, with hanging device, 110 pieces of cutlery

(Order No.: 555 510)

* All-round railing, 50 mm high
* Gusset plates as reinforcement
* Shelf reinforcing profile (No antidrumming mat in combination with the reinforcement profile)
* Air-identical castors, 4 steering castors, 2 of which have brakes; 125 mm in diameter

Panelling sets:

* Stainless-steel panelling on 3 sides, for hanging on the serving trolley, Order No.: 375449
* Panelling on 3 sides with front stainless-steel hinged doors for easy mounting on serving trolley; Order No.: 375450 (not possible in combination with gusset plates)
* Thin-sheet panelling on 3 sides, electrolytically galvanised on both sides, powder-coated in various colours; for hanging on the serving trolley; Order No.: 375453
* Thin-sheet panelling on 3 sides with front hinged doors, electrolytically galvanised on both sides, powder-coated in various colours; for easy mounting on serving trolley; Order No.: 375454 (not possible in combination with gusset plates)

Mobile work surface:

* Stainless-steel worktop WB 8 x 5 for placing on top of the serving trolley, 8 x 5 including cut-out for two GN containers 1/3-65; 2x GN 1/3-65 included in scope of delivery

(Order No.: 574 773)

* 1/1 synthetic cutting board with milled juice groove and drain into the GN containers  
  (Order No.: 574 776)
* 1/1 cutting board, made of solid beech with milled juice groove and drain into the GN containers  
  (Order No.: 574 775)
* Stainless-steel hanging frame for GN containers, including bar for paper towel roll (Order No.: 574 783)

Holds space for up to 3 Gastronorm containers GN 1/6

* Synthetic knife holder, 114x162x20 to place on GN 1/6 (Order No.: 574 774)
* Sneeze guard SW SG made of acrylic glass (PMMA), for easy mounting on tube clamps (Order No.: 574 782)
* Synthetic worktop set, comprising: Worktop WB 8x5 including 2 x GN 1/3-65, 1/1 synthetic cutting board, hanging frame, including bar for paper towel roll, 1 x GN 1/6-200, 1 x GN 1/3-200, knife holder

(Order No.: 574 778)

* Wood worktop set, comprising: Worktop WB 8x5, including 2x GN 1/3-65,

1/1 wood cutting board, hanging frame, including bar for paper towel roll, 1 x GN   
1/6-200, 1 x GN 1/3-200, knife holder

(Order No.: 574 777)

**Technical data**

Material: Stainless steel

Polyamide (PA)

Weight: 13,24 kg

Load-bearing capacity  
per trolley: 120 kg

Load-bearing capacity  
per shelf: 80 kg

Number of shelves: 2

### Special features

* All-round profile edge on the shelves to reinforce the serving trolley and prevent items on the trolley surface sliding off the sides.
* Roller-burnished shelf rim: curled edges ensure improved stability and protect staff against injury.

**Make**

Manufacturer: B.PRO

Model: SW 8x5-2

Order No.: 555 527