# CEB 53/ 37 – tray dispenser

**Dimensions**

Length: 615 mm

Width: 405 mm

Height: 765 to 865 mm

**Description**

**Structure**

The build-in tray dispenser is made entirely of CNS 18/10 (AISI 304) with a specially ground matte surface finish (“microlised” surface).

It is an open model designed for being built in. It consists of a frame construction, a base and a platform on which the trays are placed.

The platform is supported by tension springs. By hanging or unhanging individual springs, the serving height can be adjusted according to the weight of the objects stacked.

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 19,5 kg

Capacity: approx. 100 trays,

530 x 370 mm

Interior dims.: 540 x 380 mm

Emissions: The workplace-specific noise level of the unit is less than 70 dB(A)

### Special features

* protected against splash and jet water (IPX 5)
* adjustable spring tension
* complies with DIN 18665, Part 6

**Make**

Manufacturer: B.PRO

Model: CEB 53/ 37

B.PRO INMOTION

Order No.:

Installation from above: 564 022

(incl. flange)