# Storage trolley VB 75

**Dimension**

Length: 610 mm

Width: 400 mm

Height: 640 mm

**Description**

The trolley of CNS 18/10 (AISI 304) consists of a deep-drawn container, and can thus easily be cleaned. An all-round bumper profile of PUR foam protects the trolley from being damaged.

The hinged lid is removable. Each half can be opened individually. A locking device at each half of the lid guarantees that the lid does not open accidentally.

The trolley can be moved on galvanized steel castors (4 steering castors, 2 of them with brakes, castor diameter 75 mm).

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 13 kg

Capacity: 75 l (recommended)

 90 l (at maximum filling)

### Special features

* Deep-drawn container; all- round bumper profile of PU foam.

**Make**

Manufacturer: B.PRO

Model: VB 75

Order No.: 564882