**Hand-washing basin WBS 4x3.2x1.5**

**Dimensions:**

Length: 400 mm

Width: 320 mm

Height: 150/180 mm

Basin size:

Length: 340 mm

Width: 240 mm

Depth: 150 mm

**Design:**

The top surface turned down on three sides and turned up at the rear. 1 deep-drawn washbasin seamlessly welded into surface. 1 1/2" drain, with overflow protection, without valve.

With 1/2" contactless fitting (model: GIATRONIC). The temperature can be individually adjusted from cold to warm using the lever positioned at the back. The water starts automatically at the pre-selected temperature as soon as hands are placed under the fitting.

The water stops automatically when hands are removed. The transformer is installed in the lower section with a 230 V 50 HZ mains connection and corresponding connection cable. 2 stainless-steel brackets welded on. With stainless-steel basin panelling on three sides, 150 mm high.

**Technical data:**

Material: Stainless steel

Material no.: 1.4301

**Make:**

Manufacturer: B.PRO

Model: WBS 4 x 3.2 x 1.5

Order No.: 566 228