# B.PROTHERM 320 K

**Dimensions**

Length: 643 mm

Width: 430 mm

Height: 340 mm

**Description**

The food transport container is made of high-quality, physiologically safe, and food-resistant polypropylene.

The double-walled synthetic container and lid are insulated with PUR foam.

At the short sides, there are recessed stainless steel fold-out handles with ergonomically shaped synthetic grips and stainless steel clamp fasteners that grip the lid. This ensures durable closing action. The stainless steel fold-out handles are resistant to wear and tear, even under heavy use. In the inside container, there are indentations around the edge for inserting support bars securely. The safety device incorporated into the reinforced lid prevents the GN container from opening accidentally during transport.

A labelling card holder is incorporated into the top of the lid for easy identification of the food inside the container. The container is completely dishwasher safe to max. +96°C.

The interior is temperature resistant from -25°C to +100°C.

All wear and tear parts (skids and handles) are easy to exchange when servicing is necessary. All recessed screws are covered with synthetic plugs to ensure optimum hygiene.

For use with GN containers, max. size GN 1/1 – 200 mm deep or their subdivisions, inserted from above. All B.PROTHERM containers can be stacked on top of each other – even when open without lids.

The average temperature loss in closed containers is approx. 1.5°C per hour for warm food; cold foods warm up approx. 0.5°C per hour (complies with DIN EN 12571).

**Accessories / options**

* various transport trolleys and dollies—please see the general price list
* eutectic plate -3°C (order no. 569 315)
* GN support bars for variable use of GN containers (ST 3 order no. 550 650, ST 5 order no. 550 651)
* menu cards and accessories--please see the general price list

**Technical data**

Material: polypropylene (PP),

polyamide (PA), 18/10 chrome nickel steel

Insulation material: PUR foam, CFC-free

Capacity: GN 1/1-200 or their

subdivisions

Weight: 7,69 kg

### Special features

* dishwasher safe to max. +96°C
* recyclable

**Make**

Manufacturer: B.PRO

Model: BPT 320 K

B.PROTHERM

Order no. 566 241