**HAU-PW 5x6 hand-washing basin and utility sink combination, wall-mounted**

**Dimensions:**

Length: 500 mm

Width: 600 mm

Height: 570 mm

Basin size:

Length: 340 mm

Width: 240 mm

Height: 150 mm

Length: 370 mm

Width: 340 mm

Height: 150 mm

**Design:**

Hand-washing and utility sink are positioned above one another in order to save space. Consists of a compact, self-supporting design.

Can be wall-mounted using integrated brackets with hanging slot attachment system.

Both basins are equipped with three-sided stainless-steel panels with the washbasin panelling fitted at an angle. The basins are deep-drawn as one piece and are jointlessly and seamlessly welded into the top surface. The top surfaces are turned down by 50 mm on three sides. The hand-washing basin is turned up and folded by 50 mm at the back. The utility sink is equipped with a high, all-round profile edge (slosh guard).

The hand-washing basin and utility sink combination is equipped with 1 1/2" plug overflow valves and a fixed support rack made of sturdy synthetic material (material: ASA). A single-lever 3/8" mixer tap provides water in both basins. The fittings and the supply and disposal piping are not mounted when delivered but are easy to install using the operation and assembly instructions.

**Technical data:**

Material: Stainless steel

Material no.: 1.4301

**Make:**

Manufacturer: B.PRO

Model: HAU-PW 5 x 6

Order No.: 566 646