# Serving Trolley SW 6x4-3

**Dimensions**

Length: 700 mm

Width: 500 mm

Height: 950 mm

Interior dims.:

Height between shelves: 275 mm

Shelf: 600 x 400 mm

**Design**

The serving trolley consists CNS 18/10 (AISI 304),

Material No. 1.4301. Three welded-in, deep-drawn shelves are located between a stable round tube with a diameter of = 25 mm. The shelf surface is micro-polished. The round tubes on the short sides are used as push handles. A circumferential 35 mm beveled profile edge on the shelves, the roller-burnished shelf edge and one-piece welded seams between the tube frame and the shelves increase the stability of the serving trolley.

The shelves are lined underneath with a noise-insulating antidrumming mat.

The serving trolley can be moved on synthetic castors in compliance with DIN 18867, Part 8 (4 steering castors, 2 of them with locks, castor diameter 125 mm). The castors are inserted in the tube frame. Solid synthetic (polyethylene) wall guards at all four corners protect against damage.

**Accessories and options**

* Cutlery container BGN 1/3-150 of CNS, with hanging device, 110 pieces of cutlery

(Order No. 555 510)

* Circumferential railing, 50 mm high
* Gusset plates for increased stability
* Air-identical castors, 4 steering castors, 2 with brakes, diameter 125 mm

**Technical data**

Material: Chrome-nickel-steel 18/10 (AISI 304),

 Polyamide (PA)

Weight: 12,66 kg

Load-bearing capacity per trolley: 120 kg

Load-bearing capacity per shelf: 80 kg

Number of shelves: 3

### Special features

* Circumferential profile edge on shelves for increased stability of serving trolley and preventing objects placed on it from slipping off to side

**Make**

Manufacturer: B.PRO

Model: SW 6x4-3

Order No.: 569 768