# Ladle trolley LW 8 x 5-2

**Dimensions**

Length: 900 mm

Width: 600 mm

Height: 950 mm

**Description**

The ladle trolley of CNS 18/10 (AISI 304) consists of a stable 25 mm round tube construction. Between the two short sides, two deep-drawn welded-in shelves of 800 x 500 mm with all-round raised profiled edges are mounted. The upper shelf has holes for large ladles, whisks, skimmers, etc.

At the front of the upper shelf, space is provided for spice jars. A railing is mounted at both of the long sides of the upper shelf. It can be used for hanging up smaller equipment. An additional hanger bar for spoons, two-pronged meat forks, etc. is located at the front underside of the upper shelf. On the lower shelf, which serves as a dripping tray, a half-open box is installed which has holes that hold the equipment inserted from above.

The trolley has handles on both short sides.

It can be moved on stainless synthetic castors pursuant to DIN 18867, Part 8 (4 steering castors, 2 of them with brakes, castor diameter 125 mm). At all four corners, round wall bumpers are mounted.

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 19 kg

Capacity: 11 holes for ladles, whisks, etc.

### Special features

* Dripping tray with half-open box for fixing the equipment

**Make**

Manufacturer: B.PRO

Model: LW 8 x 5-2

Order No.: 569791