# Shelf Trolley RWR 161-20

**Dimensions**

Length: 663 mm

Width: 734 mm

Height: 1801 mm

Inside dimensions:

Space between support rails: 73 mm

**Design**

The shelf trolley consists of stainless steel, AISI 304. U-profile guide rails are welded between the sturdy 25 x 25 mm square tube. These are supplied with a tip safety as well as push-through protection on both sides for GN 2/1, 1/1 and 2/4.

A 20 x 10 mm square tube welded in at mid-height offset on both the front and back of the shelf trolley provides additional stability.

The shelf trolley is mobile on corrosion-resistant synthetic castors pursuant to DIN 18867, Part 8

(4 steering castors, 2 of which have brakes, castor diameter 125 mm). Synthetic (polyethylene) wall guards at all four corners protect against damage.

**Accessories/options**

* CNS paneling, 2 or 3-sided
* Transport locking bar on both sides
* Push handle short side

**Technical data**

Material: Stainless steel

Polyethylene (PE)

Material thickness  
of the square tube: 1.25 mm

Material thickness  
of the support rails: 1.25 mm

Weight: 25.0 kg

Load-bearing capacity  
per trolley: 200 kg

Number of support pairs: 20 pairs GN 1/1 or their subdivision

Capacity: 9 x GN 1/1-150 without lid

### Special features

* U-profile guide rails with push-through protection

**Make**

Manufacturer: B.PRO

Model: RWR 161-20

Order No.: 572 304