# Shelf Trolley RWR 3-A

**Dimensions**

Length: 1165 mm

Width: 625 mm

Width, including mount: 829 mm

Height: 1200 mm

Inside dimensions:

Spacing between support rails: 165 mm

**Design**

The shelf trolley consists of stainless steel, AISI 304. U-profile guide rails are welded between the sturdy 25 x 25 mm square tube. These are supplied with a tip safety as well as push-through protection.

The 3 support pairs each of the three-part trolley are used for sliding in GN containers, GN trays or GN grates. 3 GN containers can be put into position from above. The trolley is provided with a mount attached at a 10° angle, which can hold 3 GN containers (put into position from above).

The shelf trolley is mobile on corrosion-resistant synthetic castors pursuant to DIN 18867, Part 8

(4 steering castors, 2 of which have brakes, castor diameter 125 mm). Synthetic (polyamide) wall guards at all four corners protect against damage.

**Accessories/options**

* CNS panelling, 2 or 3-sided

**Technical data**

Material: Stainless steel

 Polyamide (PA)

Weight: 31 kg

Load-bearing capacity
per trolley: 80 kg

Number of support pairs: 15

Capacity: 15 x GN 1/1 or

 30 x GN 1/2

### Special features

* U-profile guide rails with push-through protection
* 6 GN containers can be put into position from above (ideal for portioning on food service conveyor belt)
* Mount attached at a 10° angle to hold 3 GN containers
* Trolley suitable for use for Cook&Chill

**Make**

Manufacturer: B.PRO

Model: RWR 3-A

Order No.: 572 308