# Basket transport trolley KWT 5 x 6

**Dimension**

Length: 664 mm

Width: 580 mm

Height: 950 mm

Platform height: 275 mm

**Description**

The basket transport trolley of CNS 18/10 (AISI 304) has a plain platform with an edge that is folded down by 60 mm on all sides. At each platform corner an aligning angle profile is mounted for stacking baskets (500 x 500 mm or 508 x 508 mm).

At one of its short sides, the trolley has a curved and slanted handle of 25 x 25 mm rectangular tube.

The trolley can be moved on stainless synthetic castors pursuant to DIN 18867, Part 8 (4 steering castors, 2 of them with brakes, castor diameter 125 mm). At all four corners, round wall bumpers are mounted.

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 10 kg

Max. load: 200 kg

Capacity: 12 baskets, each

115 mm high or 20 baskets, each 75 mm high

Dimension of basket: 500 x 500 mm or 508 x 508 mm

### Special features

* Aligning angles of round bar steel for stacking baskets. Curved handle for easy pushing

**Make**

Manufacturer: B.PRO

Model: KWT 5 x 6

Order No.: 572331