# ROLA 13 – Serving Dolly

**Dimensions**

Length: 592 mm

Width: 425 mm

Height: 535 mm

**Construction**

The serving dolly with a lid receptacle is made entirely of CNS 18/10. The surface is micro-polished.

The platform is provided with deep-drawn stacking locks which prevent the B.PROTHERM food transport container from sliding off, therefore ensuring safe transport and food serving.

Below the platform, a lock is mounted for sliding in the B.PROTHERM lid.

The stable transport frame is made of square tubing (25x25 mm).

The dolly can be moved on stainless synthetic castors pursuant to DIN 18867-8 (4 steering castors, 2 of which have brakes, with a diameter of 125 mm).

**Technical data**

Material: CNS 18/10

Weight: 10 kg

Max. load-bearing capacity: 50 kg

Capacity: 1 x BPT 160 K, or

 1 x BPT 320 ECO/ ECO-C/ K/ KB/

 KBR

**Make**

Manufacturer: B.PRO

Model: ROLA 13

Order No.: 572 341