# Potato and vegetable washing trolley KWAF 160

**Dimension**

Length: 810 mm

Width: 620 mm

Height: 750 mm

**Description**

The basin of the potato and vegetable washing trolley is deep-drawn, i. e. there are no joints where dirt could settle. Its large corner radii guarantee easy cleaning. The edge is folded down on all sides and the corners are welded. The underframe consists of a stable 25 x 25 mm rectangular tube frame construction. The basin is suitable for Gastronorm equipment, so that 4 perforated cooking inserts G-KEN G 1/1-195 mm can be used.

The 2" drain valve can be opened and closed via a tilt lever. Additional reinforcing plates are mounted above the castors.

The trolley can be moved on stainless synthetic castors pursuant to DIN 18867, Part 8 (4 steering castors, 2 of them with brakes, castor diameter 125 mm).

**Accessories and options**

* Gastronorm cooking insert G-KEN G 1/1-195 mm (Order No. 550973)
* Sieve base for dirt separation

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 21, 5 kg

Volume: 160 l

Capacity: 4 x G-KEN G 1/1-195

### Special features

* The basin is suitable for Gastronorm equipment

**Make**

Manufacturer: B.PRO

Model: KWAF 160

Order No.: 572366