# UNI-B 59/ 29 – Universal dispenser

**Dimensions**

Length: 613 mm

Width: 375 mm

Height: 765 to 865 mm

**Description**

**Structure**

The build-in universal dispenser is made entirely of CNS 18/10 (AISI 304) with a specially ground matte surface finish (“microlised” surface).

It is an closed model designed for being built in from below.

The interior is lined entirely with a powder-coated panelling to avoid marks on the crockery.

The frame of the platform has been designed so that it allows for stacking a wide variety of different types of crockery with the help of 6 synthetic guide rods that can be variably positioned.

The stacking platform runs smoothly and has ball-bearing roller guides to secure it against tilting and jamming.

The platform is supported by tension springs. By hanging or unhanging individual springs, the serving height can be adjusted according to the weight of the objects stacked.

### Accessories / options

* domed lid (640 x 340 mm), polycarbonate

stacking height w/ domed lid: 680 mm

stacking height w/o domed lid: 540 mm

* all-round flange for installation from above (order no. 572 472)

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 32 kg

Interior dims.: 590 x 290 mm

Capacity: depends on type of crockery

Emissions: The workplace-specific noise level of the unit is less than 70 dB(A)

**Special features**

* adjustable spring tension
* variable setting due to 6 guide rods
* complies with DIN 18665, Part 6

**Make**

Manufacturer: B.PRO

Model: UNI-B 59/29

 B.PRO INMOTION

Order no. 572 470