**HAU-P 5x6/900 mm hand-washing basin and utility sink combination with pedestal**

**Dimensions:**

Length: 500 mm

Width: 600 mm

Height: 900/560 mm

Basin size:

Length: 340 mm

Width: 240 mm

Height: 150 mm

Length: 370 mm

Width: 340 mm

Height: 150 mm

**Design:**

Hand-washing and utility sink are positioned above one another in order to save space. Consisting of a compact, self-supporting design that stands on four longitudinally welded square tubes (40 x 40 x 1.25 mm each). The ends of the stands are equipped with height-adjustable synthetic screw joints to compensate for floor unevenness (+/– 15 mm).

Both basins are equipped with three-sided stainless-steel panels with the washbasin panelling fitted at an angle. The basins are deep-drawn as one piece and are jointlessly and seamlessly welded into the top surface. The top surfaces are turned down by 50 mm on three sides. The hand-washing basin is turned up and folded by 50 mm at the back. The utility sink is equipped with a high, all-round profile edge (slosh guard).

The hand-washing basin and utility sink combination is equipped with 1 1/2" plug overflow valves and a fixed support rack made of sturdy synthetic material (material: ASA). A single-lever 3/8" mixer tap provides water in both basins. The fittings and the supply and disposal piping are not mounted when delivered but are easy to install using the operation and assembly instructions.

**Accessories/options:**

* Waste drawer:

The waste drawer is available for all HAU-P and HAU-PS models.

It is positioned beneath the utility sink and can be opened and closed

with the foot. The waste container comprises a B.PRO GN container with D-shaped handles – GN-B 2/3-150 – which can be easily removed for cleaning.

* Removable maintenance panel
* Swingaway support rack made of stainless steel (instead of synthetic fixed support rack)

**Technical data:**

Material: Stainless steel

Material no.: 1.4301

**Make:**

Manufacturer: B.PRO

Model: HAU-P 5 x 6/900 mm

Order No.: 572 553