HAU-PS 5x6/900 mm hand-washing basin and utility sink combination, sensor controlled with pedestal

**Dimensions:**

Length: 500 mm

Width: 600 mm

Height: 900/560 mm

Basin size:

Length: 340 mm

Width: 240 mm

Height: 150 mm

Length: 370 mm

Width: 340 mm

Height: 150 mm

**Design:**

Hand-washing and utility sink are positioned above one another in order to save space. Consisting of a compact, self-supporting design that stands on four longitudinally welded square tubes (40 x 40 x 1.25 mm each). The ends of the stands are equipped with height-adjustable synthetic screw joints to compensate for floor unevenness (+/– 15 mm).

Both basins are equipped with three-sided stainless-steel panels, and the diagonal panelling of the washbasin is removable. The basins are deep-drawn as one piece and are jointlessly and seamlessly welded into the top surface. The top surfaces are turned down by 50 mm on three sides. The hand-washing basin is turned up and folded by 50 mm at the back. The utility sink is equipped with an all-round profile edge (slosh guard).

The hand-washing basin and utility sink combination is equipped with 1 1/2" plug overflow valves and a fixed support rack made of sturdy synthetic material (material: ASA). The hand-washing basin is equipped with a 1/2" contactless fitting (model: Aquis). The lever on the side can be used to adjust the temperature between hot and cold as required. As soon as the hands are held under the fitting, the water flows automatically at the pre-selected temperature. When the hands are removed, the water flow stops. The transformer is installed in the lower area with a mains connection of 230 V/50 HZ and corresponding connection cable.

The manually adjustable 1/2" single-lever mixer tap for the utility sink is also equipped for assembly on the hand-washing basin.

The supply and disposal piping, along with the fittings, are supplied loose and are easy to install following the operation and assembly instructions.

**Accessories/options:**

* Waste drawer:

The waste drawer is available for all HAU-P and HAU-PS models.

 It is positioned beneath the utility sink and can be opened and closed with the foot.

 The waste container comprises a B.PRO GN container with D-shaped handles – GN-B 2/3-150 – which can be easily removed for cleaning.

* Swingaway support rack made of stainless steel (instead of synthetic fixed support rack)
* Selectively controlled battery-operated mixer tap instead of mains connection (battery-operated with 3 V battery)

Dual infrared sensor with fully automatic setting; fitted with non-return valve and pre-assembled strainer; permanent-on and hygiene flush adjustable with click button; max. water temperature 80 °C, adjustable hot water flow restrictor; brief-off (cleaning) and permanent-on (filling) activated with click button.

**Technical data:**

Material: Stainless steel

Material no.: 1.4301

Elec. Connected load: 230 V/50 HZ

**Make:**

Manufacturer: B.PRO

Model: HAU-PS 5 x 6/900 mm

Order No.: 572 554