# RWRA 851 Shelf Trolley

**Dimensions**

Length: 662 mm

Width: 733 mm

Height: 845 mm

Interior dimensions:

Space between support rails: 73 mm

**Design**

The shelf trolley consists of CNS 18/10 (AISI 304), Material No. 1.4301. U-profile guide rails are welded between the stable 25 x 25 mm square tubes. These are supplied with a tip safety as well as push-through protection on both sides for GN 2/1, 1/1 and 2/4. The shelf trolley is equipped with a smooth work surface (590 x 662 mm), which

is turned down on 4 sides.

The shelf trolley can be moved on corrosion- resistant synthetic castors (4 steering castors, 2 of which have locking brakes, castor diameter 125 mm). Solid synthetic (polyamide) wall guards at all four corners protect against damage.

**Accessories and options**

* CNS paneling, 2 or 3-sided
* Transport circlip, double-sided

**Technical data**

Material: Chrome-nickel-steel 18/10 (AISI 304),

Polyamide (PA)

Material thickness

of the square tube: 1.5 mm

Material thickness of

the support rails: 1.2 mm

Weight: 20 kg

Load-bearing capacity

per trolley: 200 kg

Number of support

pairs: 8 pairs GN 1/1 or their subdivision

Capacity: 4 x GN 1/1-150 without lid

### Special features

* U-profile guide rails with tip safety and push-through protection on both sides
* Model with a work surface
* For rolling under open work tables

**Make**

Manufacturer: B.PRO

Model: RWRA 851

Order No.: 572 928