# RWRA 852 Shelf Trolley

**Dimensions**

Length: 820 mm

Width: 613 mm

Height: 845 mm

Interior dimensions:

Space between support rails: 73 mm

**Design**

The two-part shelf trolley consists of CNS 18/10 (AISI 304), Material No. 1.4301. U-profile guide rails are welded between the stable 25 x 25 mm square tubes. These are supplied with a tip safety as well as push-through protection on both sides for GN 2/1, 1/3 and 2/8. The shelf trolley is equipped with a smooth work surface (748 x 542 mm) which is turned down on 4-sides.

The shelf trolley can be moved on galvanized steel castors (4 steering castors, 2 of which have locking brakes, castor diameter 125 mm). Solid synthetic (polyamide) wall guards at all four corners protect against damage.

**Accessories and options**

* CNS paneling, 2 or 3-sided
* Transport circlip, double-sided

**Technical data**

Material: Chrome-nickel-steel 18/10 (AISI 304), Polyamide (PA)

Material thickness of the

square tube: 1.5 mm

Material thickness of the

support rails: 1.2 mm

Weight: 22 kg

Load-bearing capacity

per trolley: 180 kg

Number of support pairs: 16 (2 x 8) pairs GN 1/1 or their subdivision

Capacity: 8 x GN 1/1-150 without lid

### Special features

* U-profile guide rails with tip safety and push-through protection on both sides
* 2-part design with work surface
* For rolling under open worktables

**Make**

Manufacturer: B.PRO

Model: RWRA 852

Order No.: 572 929