# RWR 162 Shelf Trolley

**Dimensions**

Length: 820 mm

Width: 613 mm

Height: 1645 mm

Interior dimensions:

Space between support rails: 73 mm

**Design**

The shelf trolley consists of CNS 18/10 (AISI 304), Material No. 1.4301. U-profile guide rails are welded between the stable 25 x 25 mm square tubes (curved without a recess). These are supplied with a tip safety as well as push-through protection on both sides for GN 2/1, 1/3 and 2/8. The shelf trolley is two-part.

A 20 x 10 mm square tube welded in elevated at mid-height on both the front and back of the shelf trolley provides additional stability.

The shelf trolley can be moved on galvanized steel

castors (4 steering castors, 2 of which have locking brakes, castor diameter 125 mm). Solid synthetic (polyamide) wall guards at all four corners protect against damage.

**Accessories and options**

* Dust protection hood made of transparent polyethylene (Order No. 568 773)
* Insulating hood made of polyethylene, aluminized on both sides (Order No. 568 776)
* Trolley top made of CNS
* CNS paneling, 2 or 3-sided
* Transport circlip, double-sided
* Push handle

**Technical data**

Material: Chrome-nickel-steel 18/10 (AISI 304),

 Polyamide (PA)

Material thickness of the

square tube: 1.5 mm

Material thickness of the

support rails: 1.2 mm

Weight: 29 kg

Load-bearing capacity

per trolley: 200 kg

Number of support

pairs: 36 pairs GN 1/1 or their subdivision

Capacity: 17 x GN 1/1-150 without lid

### Special features

* U-profile guide rails with tip safety and push-through protection on both sides
* 2-part model

**Make**

Manufacturer: B.PRO

Model: RWR 162

Order No.: 572 941