# Shelf Trolley RWR SK-161

**Dimensions**

Length: 662 mm

Width: 733 mm

Height: 1645 mm

Interior dimensions:

Space between support rails (top): 115 mm

Interior dimensions:

Space between support rails (bottom): 73 mm

**Design**

The shelf trolley consists of CNS 18/10 (AISI 304), Material No. 1.4301. 5 pairs of U-profile guide rails are welded between the stable 25 x 25 mm square tubes, mounted diagonally at approx. 10°. These are supplied with a tip safety as well as push-through protection on both sides. Below these are 9 pairs of horizontally mounted support rails, which are supplied with a tip safety and push-through protection on both sides.

5 serving doors for salads and desserts are attached at the front of the top 5 pairs of support rails.

The shelf trolley can be moved on galvanized steel castors (4 steering castors, 2 of which have locking brakes, castor diameter 125 mm). Solid synthetic (polyamide) wall guards at all four corners protect against damage.

**Technical data**

Material: Chrome-nickel-steel 18/10 (AISI 304),

Polyamide (PA)

Material thickness of the square tube: 1.5 mm

Material thickness of the

support rails: 1.2 mm

Weight: 30 kg

Load-bearing capacity per trolley: 200 kg

Number of support

pairs (diagonal): 5

Number of support

pairs (horizontal): 9

Capacity: 14 x GN 2/1-20, or

14 x BZG 2/1-20

### Special features

* 9 pairs of horizontally mounted U-profile guide rails with tip safety and push-through protection on both sides
* 5 pairs of diagonally (approx. 10°) mounted support rails with tip safety and push-through protection on one side
* Salad and dessert serving trolley

**Make**

Manufacturer: B.PRO

Model: RWR SK-161

Order No.: 572 943