**BASIC LINE N-3 plain buffet with smooth top surface**

**Dimensions:**

Length: 1254 mm

Width 1: 770 mm

(= with folded-down tray slide on guest side)

Width 2: 990 mm

(= with folded-up tray slide on guest side)

*Width 3: 1302 mm*

*(= with folded-up tray slide on guest and operator side: serving from both sides possible)*

Height of top surface: 900 mm

Height including heat bridge: 1305 mm

*Alternative overall height for self-serve children's catering:*

*Height of top surface: 750 mm*

*Height including heat bridge: 1155 mm*

*(The range of accessories described in the following cannot be completely offered with a reduced overall height.)*

**Basic buffet:**

Mobile buffet, based on a sturdy, self-supporting sheet-metal structure, installed ready to plug in, with approx. 2 m connection cable and plug.

**Top surface:**

The plain buffet is equipped with a 40 mm high top surface of micro-polished stainless steel with smooth bevelling on all sides. An approx. 240 mm high trim panel is located below the top surface on both long sides.

**Tray slide:**

The folding brackets of stainless-steel sheet for the stainless-steel round-tube tray slide are mounted below the stainless-steel top surface on the two flanks for the side faces on the guest side. Tube diameter: 25 mm. Height of upper edge of round-tube tray slide: 885 mm.

**Underframe:**

The side faces and the trim panels below the stainless-steel top surface on the guest and operator side are made of powder-coated thin sheet electrolytically galvanised on both sides. The standard colour of the basic buffet below the stainless-steel top surface:

Stone grey (RAL 7030)

*As an alternative, the following colours are available for the underframe:* See B.PRO BASIC LINE accessories/colour options \*

The castors are mounted on the underside of the side faces: 2 twin steering castors with brakes on the operator side, 2 twin steering castors on the guest side, castor diameter: 75 mm.

**Accessories/options:**

* Sneeze guard made of ESG safety glass on customer side, bridge attachment made of stainless steel, pass-through height 275 mm
* Sneeze guard on operator side also available as an option
* Sneeze guard made of ESG safety glass with lighting on customer side, bridge attachment made of stainless steel, with fluorescent tubes, pass-through height 275 mm
* Sneeze guard on operator side also available as an option
* Sneeze guard made of ESG safety glass on customer side, bridge attachment made of stainless steel with 3 individually switchable ceramic radiators (250 W each), pass-through height 275 mm
* Sneeze guard on operator side also available as an option
* Optionally also with lighting, 2 low-voltage halogen lamps (20 W each), can be swivelled
* Opening for cable bushing, centrally in middle of stainless-steel top surface.
* Tray slide made of stainless-steel round tube (25 mm tube diameter) on operator side, fold-down. At standard height (885 mm) or reduced height (785 mm) for children's catering.
* Shelf made of stainless-steel round tube (25 mm tube diameter) on short side right and/or left, fold-down. At standard height (885 mm) or reduced height (785 mm) for children's catering.
* Plate slide made of stainless-steel sheet (200 mm wide) on customer side and/or operator side, fold-down. Flush with the top surface at height of 900 mm.
* Tray slide made of stainless-steel sheet (280 mm wide) on customer side and/or operator side, fold-down. At standard height (885 mm) or reduced height (785 mm) for children's catering.
* Shelf made of stainless-steel sheet (340 mm wide) on short side right and/or left, fold-down. Flush with the top surface (900 mm) or at standard height (885 mm) or reduced height (785 mm) for children's catering.
* Additional socket outlets. Two additional socket outlets with 230 V Schuko each, on operator side installed on inside of right side face. Power consumption increased by 2 x 3.5 kW / 400 V / 3N PE
* Stainless-steel base bottom, for adjusting B.PROTHERM BPT 420 K / KBUH / KBRUH
* Module connectors for permanent connection of two buffets
* Feet made of stainless steel (instead of castors)
* Stainless-steel skirting panels on customer side/short side right/left (can only be ordered in conjunction with feet)
* Profile panel for customer-side concealment of the gap between two modules, does not replace the module connector (can only be ordered in combination with skirting panels and module connectors).
* Underframe coating: Side faces & panels powder-coated in colours of B.PRO BASIC LINE \*
* Front panelling on customer and operator side, between side faces, easy to remove and mount
* made of thin sheet, electrolytically galvanised on both sides, powder-coated in B.PRO BASIC LINE colours. \*
* or micro-polished stainless-steel sheet.
* or particle board, coated with RESOPAL laminate
* B.PRO BASIC LINE colours: \*

signal white, RAL 9003

pearl white, RAL 1013

pale brown, RAL 8025

stone grey, RAL 7030

umbra grey, RAL 7022

graphite black, RAL 9011

broom yellow, RAL 1032

carmine red, RAL 3002

sapphire blue, RAL 5003

raspberry, Pantone 228 C

lime, Pantone 382 C

espresso, Pantone 4695 C

apple green, Pantone 370 C

Other colours on request

**Technical data:**

Material: Stainless steel (AISI 304), micro-polished; combined with powder-coated, thin sheet electrolytically galvanised on both sides.

Weight: approx. 65 kg (without options)

Capacity: same as 3 x GN 1/1

Connected load: ---

*With optional accessories, a new connected load results for the buffet.*

*Example optional additional socket outlets and heat bridge / light bridge*

New connected load:400 V / 16 A / 3N PE / 50‑60 Hz / max. 8 kW / CEE plug.

**Special features:**

* Sneeze guard made of ESG safety glass
* Micro-polished surface made of stainless steel
* Fold-down tray slide made of stainless-steel round tube and stainless-steel sheet
* Wide selection of colour design options

**Make:**

Manufacturer: B.PRO

Type: BASIC LINE N-3

Order No.: 573 077