**Convection-cooled showcase attachment, glass-enclosed on guest side**

**Dimensions:**

Outside length: 1,410 mm

Inside length: 1,100 mm

Outside width: 508 mm

Inside width: 450 mm

Outside height: 700 mm

Inside height: 605 mm

Insertion dimensions with window open: 530 x 600 mm

**Design:**

Convection-cooled showcase attachment, glass-enclosed on 3-sides; serving side with 2 insulated sliding glass windows, insulated glass on customer side; intake side is customer side, exhaust side is serving side; machine compartment attached on left from serving side; outside and inside panelling of chrome nickel steel 1.4301; insulation 40 mm polyurethane, FC and CFC-free; refrigeration technology with convection cooling ready to plug in; thermostat with digital temperature display, automatic defrosting and condensed water evaporation; bright interior lighting mounted on cover; 2 adjustable CNS fixed, perforated support racks for optimised air guidance in interior.

**Technical data:**

Material: Chrome nickel steel 18/10 (WN 1.4301/AISI 304), micro-polished.

Weight: approx. 108 kg

Net capacity: approx. 302 litres

Temperature range: +4°C to +12°C at +32°C ambient temperature und 60% rel. humidity

Evaporating

temperature: -10°C

Refrigerant: R 134 A (300 g)

Cooling capacity: 290 W at -10°C evap. temperature

Energy consumption: 3.4 kWh/24 hrs.

Connected load: 220-240V/16 A/1N PE/50 Hz/

0.24 kW/Schuko plug.

**Make:**

Manufacturer: B.PRO GmbH + Co.KG

Model: AKV-S 147

Order No.: 573 206