# Shelf trolley RWR 3-A KS

**Dimensions**

Length: 1,180 mm

Width: 823 mm

Height: 1,200 mm

Space between support rails: 82 mm

**Model**

The shelf trolley consists of AISI 304. U-profile guide rails are welded between the sturdy 25 x 25 mm square tube. These are supplied with a tip safety as well as push-through protection.

The 7 support pairs each of the three-part trolley are used for sliding in GN containers, GN trays or GN grates. In addition, 3 GN containers of the size GN 1/1 can be hooked in from above. The trolley is provided with an attachment mounted at a 10° angle, which can hold 3 GN containers of the size GN 1/1 (hooked in from above).

To prevent cold loss, the shelf trolley has a one-piece stainless steel bottom plate

The shelf trolley is mobile on galvanised steel castors (4 steering castors, 2 of which have brakes, castor diameter 125 mm). Synthetic (polyamide) wall guards at all four corners protect against damage.

**Technical data**

Material: AISI 304

 Polyamide (PA)

Weight: 38 kg

Load-bearing capacity

per trolley: 200 kg

Number of support pairs: 3 x 7 pieces

Capacity: 27 x GN 1/1 or

 54 x GN 1/2

### Special features

* U-profile guide rails with tip safety and push-through protection
* 3x GN containers of the size GN 1/1 can be hooked in from above (ideal for portioning on food service conveyor belt)
* Attachment mounted at a 10° angle for holding 3 GN containers of the size GN 1/1

**Make**

Manufacturer: B.PRO

Type: RWR 3-A KS

Order No.: 573387