# Cutlery and tray trolley BT 400

**Dimension**

Length: 900 mm

Width: 600 mm

Height: 1270 mm

**Description**

The cutlery and tray trolley of CNS 18/10 (AISI 304) has a slanted top unit with 5 CNS cutlery containers of size GN 1/4-150. The short sides of the top unit are entirely covered with plastic panellings. The chassis consists of a stable construction of curved 25 x 25 mm rectangular tube with a bottom shelf which serves as a tray support. The shelf is welded-in and its back edge is folded up by 50 mm (glide stop).

For sanitary reasons, all cutlery containers are equipped with transparent Plexiglas half flap covers. The bottoms of the containers are slanted, so that the cutlery can easily be taken out. The last cutlery container can be divided vertically to separate cake forks and coffee spoons.

The trolley can be moved on galvanized steel castors (4 steering castors, 2 of them with brakes, castor diameter 125 mm). At all four corners, round wall bumpers are mounted.

**Accessories**

* Additional shelf

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 21 kg

Capacity: approx. 120 Gastronorm or Euronorm trays, approx. 500 pieces of cutlery

**Make**

Manufacturer: B.PRO

Model: BT 400

Order No.: 573415