# Cutlery and tray trolley BT 800

**Dimension**

Length: 900 mm

Width: 600 mm

Height: 1485 mm

**Description**

The cutlery and tray trolley of CNS 18/10 (AISI 304) has a slanted top unit with 10 CNS cutlery containers of size GN 1/4-150. The short sides of the top unit are entirely covered with plastic panellings. The chassis consists of a stable construction of curved 25 x 25 mm rectangular tube with a bottom shelf which serves as a tray support. The shelf is welded-in and its back edge is folded up by 50 mm (glide stop).

For sanitary reasons, all cutlery containers are equipped with transparent Plexiglas half flap covers. The bottoms of the containers are slanted, so that the cutlery can easily be taken out. The last cutlery container can be divided vertically to separate cake forks and coffee spoons.

The trolley can be moved on galvanized steel castors (4 steering castors, 2 of them with brakes, castor diameter 125 mm). At all four corners, round wall bumpers are mounted.

**Options**

* Version with total height of 1120 mm available for child / school catering

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 35 kg

Capacity: approx. Gastronorm or Euronorm 120 trays, approx. 1100 pieces of cutlery

**Make**

Manufacturer: B.PRO

Model: BT 800

Order No.: 573417