# Serving Trolley SW 8x5-2

**Dimensions**

Length: 900 mm

Width: 600 mm

Height: 950 mm

Interior dims.:

Height between shelves: 585 mm

Shelf: 800 x 500 mm

**Design**

The serving trolley consists CNS 18/10 (AISI 304),

Material No. 1.4301. Two welded-in, deep-drawn shelves are located between a stable round tube with a diameter of = 25 mm. The shelf surface is micro-polished. The round tubes on the short sides are used as push handles. A circumferential 35 mm beveled profile edge on the shelves, the roller-burnished shelf edge and one-piece welded seams between the tube frame and the shelves increase the stability of the serving trolley.

The shelves are lined underneath with a noise-insulating antidrumming mat.

The serving trolley can be moved on 4 air-identical steering castors, 2 of them with locks, castor diameter 125 mm. The castors are inserted in the tube frame. Solid synthetic (polyethylene) wall guards at all four corners protect against damage.

**Accessories and options**

* Garbage container AFB 4 x 2 x 2.5 of CNS, with hanging device, 18.5 liters (Order No. 555 509)
* Cutlery container BGN 1/3-150 of CNS, with hanging device, 110 pieces of cutlery

(Order No. 555 510)

* Circumferential railing, 50 mm high
* Gusset plates for increased stability
* Shelf reinforcement profiles (No antidrumming mat in combination with the reinforcement profile)

Panelling sets:

* Panelling 3-sided, stainless steel, for hooking on serving trolleys, Order No.: 375449
* Panelling 3-sided with hinged doors on the front, stainless steel, for easy mounting to serving trolleys, Order No.: 375450 (not possible in combination with gusset plates)
* Panelling 3-sided, thin sheet, galvanized double-sided, powder-coated in various colours, for hooking on serving trolleys, Order No.: 375453
* Panelling 3-sided with hinged doors on the front, thin sheet, galvanized double-sided, powder-coated in various colours, for easy mounting to serving trolleys, Order No.: 375454 (not possible in combination with gusset plates)

Mobile work surface:

* Stainless-steel worktop WB 8 x 5 for placing on top of the serving trolley, 8 x 5 including cut-out for two GN containers 1/3-65; 2x GN 1/3-65 included in scope of delivery

(Order No.: 574 773)

* 1/1 synthetic cutting board with milled juice groove and drain into the GN containers
(Order No.: 574 776)
* 1/1 cutting board, made of solid beech with milled juice groove and drain into the GN containers
(Order No.: 574 775)
* Stainless-steel hanging frame for GN containers, including bar for paper towel roll (Order No.: 574 783)

Holds space for up to 3 Gastronorm containers GN 1/6

* Synthetic knife holder, 114x162x20 to place on GN 1/6 (Order No.: 574 774)
* Sneeze guard SW SG made of acrylic glass (PMMA), for easy mounting on tube clamps (Order No.: 574 782)
* Synthetic worktop set, comprising: Worktop WB 8x5 including 2 x GN 1/3-65, 1/1 synthetic cutting board, hanging frame, including bar for paper towel roll, 1 x GN 1/6-200, 1 x GN 1/3-200, knife holder

(Order No.: 574 778)

* Wood worktop set, comprising: Worktop WB 8x5, including 2x GN 1/3-65,

1/1 wood cutting board, hanging frame, including bar for paper towel roll, 1 x GN
1/6-200, 1 x GN 1/3-200, knife holder

(Order No.: 574 777)

**Technical data**

Material: Chrome-nickel-steel 18/10 (AISI 304)

 Polyamide (PA)

Weight: 12,5 kg

Load-bearing capacity per trolley: 120 kg

Load-bearing capacity per shelf: 80 kg

Number of shelves: 2

### Special features

* Circumferential profile edge on shelves for increased stability of serving trolley and preventing objects placed on it from slipping off to side

**Make**

Manufacturer: B.PRO

Model: SW 8x5-2

Order No.: 573 476