# Serving trolley SW 10x6-3 BASIC

**Dimensions**

Length: 1100 mm

Width: 700 mm

Height: 950 mm

Inside dimensions:

Height between shelves: 275 mm

Shelves: 1000 x 600 mm

**Design**

Serving trolley SW 10x6 in basic design.

The serving trolley is made of stainless steel,   
AISI 304. There are three welded-in, deep-drawn shelves between a sturdy round tube 25 mm in diameter. The shelf surfaces are micro-polished. The round tubes on the short sides are used as push handles. A 35-mm turned-down, all-round profile edge on the shelves, the roller-burnished shelf rim and single-piece welded seams between the tube frame and shelves all make the serving trolley sturdier.

A noise-insulating anti-drumming mat is positioned beneath the shelves.

The serving trolley can be moved on synthetic castors in compliance with DIN 18867, Part 8 (4 steering castors, 2 of them with locks, castor diameter 125 mm). The castors are inserted into the tube frame. Synthetic (polyethylene) wall guards at all four corners protect against damage.

**Accessories/options**

* Stainless-steel cutlery attachment CAT 5, including 5 GN 1/4-150 cutlery holders with transparent, half-flap Plexiglas top surface,   
  500 pieces of cutlery. For easy mounting on tube clamps (Order No.: 574 772)
* Stainless-steel waste container AFB 4 x 2 x 2.5, with hanging device, 18.5 litres (Order No.: 555 509)
* Stainless-steel cutlery holder BGN 1/3-150, with hanging device, 110 pieces of cutlery

(Order No.: 555 510)

* All-round railing, 50 mm high
* Gusset plates as reinforcement
* Shelf reinforcing profile (No antidrumming mat in combination with the reinforcement profile)
* Air-identical castors, 4 steering castors, 2 of which have brakes; 125 mm in diameter

Panelling sets:

* Stainless-steel panelling on 3 sides, for hanging on the serving trolley, Order No.: 375451
* Panelling on 3 sides with front stainless-steel hinged doors for easy mounting on serving trolley; Order No.: 375452 (not possible in combination with gusset plates)
* Thin-sheet panelling on 3 sides, electrolytically galvanised on both sides, powder-coated in various colours; for hanging on the serving trolley; Order No.: 375455
* Thin-sheet panelling on 3 sides with front hinged doors, electrolytically galvanised on both sides, powder-coated in various colours; for easy mounting on serving trolley; Order No.: 375456 (not possible in combination with gusset plates)

**Technical data**

Material: Stainless steel

Polyamide (PA)

Weight: 20,8 kg

Load-bearing capacity  
per trolley: 120 kg

Load-bearing capacity  
per shelf: 80 kg

Number of shelves: 3

### Special features

* All-round profile edge on the shelves to reinforce the serving trolley and prevent items on the trolley surface sliding off the sides.
* Roller-burnished shelf rim: curled edges ensure improved stability and protect staff against injury.

**Make**

Manufacturer: B.PRO

Model: SW 10x6-3 BASIC

Order No.: 573488