# Serving Trolley SW 10x6-4 BASIC

**Dimensions**

Length: 1100 mm

Width: 700 mm

Height: 1290 mm

Interior dimension:

Height between shelves: 285 mm

Shelves : 1000 x 600 mm

**Model**

Serving trolley SW 10x6 in basic design.

The serving trolley consists CNS 18/10, Material No. 1.4301. Four welded-in, deep-drawn shelves are located between a stable round tube with a diameter of = 25 mm. The shelf surface is micro-polished. The round tubes on the short sides are used as push handles. A circumferential 35 mm bevelled profile edge on the shelves, the roller-burnished shelf edge and one-piece welded seams between the tube frame and the shelves increase the stability of the serving trolley.

The shelves are lined underneath with a noise-insulating antidrumming mat.

The serving trolley can be moved on galvanised steel castors (4 steering castors, 2 of which have brakes, castor diameter 125 mm). The castors are inserted in the tube frame. Solid synthetic (polyethylene) wall guards at all four corners protect against damage.

**Accessories/options**

* Garbage container AFB 4 x 2 x 2.5 of CNS, with hanging device, 18.5 litres (Order No. 555 509)
* Cutlery container BGN 1/3-150 of CNS, with hanging device, 110 pieces of cutlery

(Order No. 555 510)

* All-round railing, 50 mm high
* Gusset plates for increased stability
* Shelf reinforcement profiles (No antidrumming mat in combination with the reinforcement profile)
* Air-identical castors, 4 steering castors, 2 with brakes, diameter 125 mm

**Technical data**

Material: Chrome-nickel-steel 18/10,

Polyamide (PA)

Weight: Approx. 34 kg

Load-bearing capacity per trolley: 120 kg

Load-bearing capacity per shelf: 80 kg

Number of shelves: 4

### Special features

* Circumferential profile edge on shelves for increased stability of serving trolley and preventing objects placed on it from slipping off to side

**Make**

Manufacturer: B.PRO

Model: SW 10x6-4 BASIC

Order No.: 573491