# Tray transport trolley

# double-walled model, for passive cooling with eutectic plates

# TTW-PK 30-115 DDE

**Dimensions**

Length: 1554 mm

Width: 783 mm

Height: 1636 mm

**Design**

**Design**

The trolley body is closed on all sides and made completely of stainless steel. The surface is micro-polished. The edged bottom panel is reinforced with longitudinal profiles on the underside. The doors are double-walled and insulated with polystyrene hard foam plates. Additional insulation on the top and unit bottom ensures lower temperature loss in the interior. Interior and exterior body are vertically connected with synthetic profiles and thermally separated.

Side and dividing walls in the compartment are designed for holding trays with seamless deep-drawn support ledges spaced 115 mm apart. To prevent accidental tipping when pulling out trays, two seamlessly deep-drawn tip safety mechanisms are provided above the tray supports with a spacing of   
7 mm. The support ledges have a width of 11.5 mm for safely holding Euronorm trays (530 x 370 mm). The self-supporting design enables use both inside and outside the building.

There are two holders for eutectic plates on the inside of each of the two doors. The holders consist of two support frames and one condensation-water catch tray. The lower support frame and the condensation-water catch tray are designed as a single component. This ensures that the catch trays are always used. Because the eutectic plates are portioned on the inside of the doors, each compartment is cooled separately. The individual compartments can be opened independently from one another.

The left and right hinged doors can be opened by 270°. The doors for the middle compartment can be opened by 180°. All doors can be securely locked using a spring-loaded synthetic moulded part on the bottom of the tray transport trolley. The doors locked in the open position are located within the bumper rail to prevent damage. In addition, the doors have an all-round removable silicone seal profile to prevent temperature losses.

The door lock mounted vertically in the middle of the doors is self-closing and designed with an integrated transport security. The sturdy door hinges are welded and protected against impacts, as they are located within the bumper rail.

**Use/ergonomics**

The tray transport trolley is designed to transport portioned food on trays – especially for early portioning of evening meals.

It is equipped with a sturdy all-round bumper rail, which protects the trolley from damage. Two vertical, ergonomically positioned push handles are located on both short sides. The push handles are located within the bumper rail to prevent the hands from being pinched when rolling through doors and narrow corridors. The push handles are accessible even with the door open.

The tray transport trolley can be moved on 2 fixed castors and 2 steering castors with brakes, a diameter of 160 mm and a galvanised steel housing.

### Special features

* Self-closing door locks with integrated transport security
* Doors with removable all-round seal profile
* Interior and exterior body are vertically connected with synthetic profiles and thermally separated
* Holders for eutectic plates on the inside of the doors

##### Technical data

Material: Stainless steel, AISI 304,

Polyethylene (PE)

Insulating material

Doors, walls, top

and unit bottom: Polystyrene hard foam plates (30 mm)

Weight: approx. 179 kg

Capacity: 30 EURONORM trays   
(530 x 370 mm)

Insertion type: lengthwise

Number of holders

for eutectic plates: 6

Spacing of

support ledges: 115 mm

Spacing of

tip safety/ledges: 7 mm

Number of   
compartments: 3

Number of   
hinged doors: 3

Interior design: HS hygienic type,

pursuant to DIN 18865-9

**Accessories/options**

* Eutectic plate (-3°C) made of synthetic, Order No.: 568136)
* Eutectic plate (-12°C) made of synthetic, Order No.: 573332)
* All-round bumper rail, milled
* Additional bumper rail on top
* All-round railing, with mitred welding
* Draw bar and coupling
* Antistatic conveyor
* Castor diameter is 200 mm
* Stainless-steel castors with elastic castors
* Castor arrangement D with central locking brake

**Make:**

Manufacturer: B.PRO

Model: TTW-PK 30-115 DDE

Order No.: 573731