# Plate dispenser TSE-1 18-33 ET 630

# (for installation)

**Dimensions**

Length: 425 mm

Width: 425 mm

Height: (incl. plate guides) 760 mm

**Model**

The plate dispenser for installation is completely designed in AISI 304 and consists of one square plate tube. The plate tube has a particularly flat stacking platform with jam-proof guides.

Using four Rilsan-coated plate guide rods, it can be adjusted to various plate sizes and plate shapes flexibly and without tools using a hole pattern on the bottom. For example, round plates with a diameter of 18 – 33 cm and rectangular plates up to a maximum of 28 x 28 cm can be stacked in the plate tube.

The plate guide rods project above the flange ring of the dispenser. This means that more plates can be securely unstacked with it.

To ensure a consistently even serving height, the spring tension can be regulated depending on the stacked items by hooking or unhooking the tension springs.

This setting can be made quickly and effortlessly because of special cut-outs in the spring retainers.

### Accessories/options

* Transparent polycarbonate hooded cover
* Insulated hooded cover made of EPP, silver-grey
* Refilling signal

(The refilling signal shows the personnel in time when the plates in the corresponding tube are running low.)

* 4 additional plate guides per tube

(Using the additional plate guides, 4 stacks of small dishes such as soup dishes or salad and dessert bowls can be stacked in the plate tube. Also, the additional plate guides support stacks of unusually shaped plates)

**Technical data**

Material: AISI 304

Weight: approx. 13 kg

Max. load: 65 kg

Capacity: approx. 70 plates (depending on the stacking height)

Dish dimensions: Round: 18-33 cm dia.

Rectangular:   
 max. 28x28 cm

Installation depth: 630 mm

Worktop cut-out: (see drawing for cut-out dimensions)

Number of tubes: 1

Stacking height with

hooded cover: 685 mm

Stacking height w/o

hooded cover: 670 mm

Emissions: The workplace-specific noise level of the unit is less than 70 dB(A)

### Special features

* Large, square plate tube for a high level of flexibility in loading various plate sizes and plate shapes
* Particularly flat, stacking platform with jam-proof design
* High guide rods to hold the plates securely, even without a hooded cover
* Simple spring setting due to the Easy-Set System

**Make**

Manufacturer: B.PRO

Type: TSE-1 18-33 ET 630

Order No.: 573780