# B.PROTHERM BPT 320 ECO-C

**Dimensions**

Length: 630 mm

Width: 415 mm

Height: 345 mm

**Model**

The food transport container is made of high-quality, non-hazardous, food-resistant polypropylene.

The double-walled synthetic container and lid are filled with PUR foam for thermal insulation.

The interior container of the BPT 320 ECO-C is designed in such a way that several GN containers of the size 1/1 or its subdivisions can be stacked one on top of another.

The BPT 320 ECO-C features cut-outs in the four corner areas and on both long sides. These cut-outs make it easier to remove and insert the GN containers.

The bottom of the interior container has moulded bars which also have a positive impact on the insulating properties when GN containers are inserted.

The practical clamped lid is easy to open and close.

One device for holding marking cards is integrated into each of the short sides of the container to identify the food in the container. The container is completely dishwasher-safe up to a maximum of +96°C. The unit interior is resistant to temperatures from -25°C to +100°C.

The Gastronorm containers are loaded from the top. The container is designed for the following loading with GN 1/1 or its subdivisions:

* 4x GN 1/1-55 (or subdivisions)
* 3x GN 1/1-65 (or subdivisions)
* 2x GN 1/1-100 (or subdivisions)
* 1x GN 1/1-200 (or subdivisions)

All B.PROTHERM containers can be stacked with one another, even when open without a lid.

The average temperature loss of hot and cold food with the container closed fulfils the requirements of DIN EN 12571.

### Accessories/options

* Various transport trolleys and dollies according to the full price list
* GN slide-in frame (Art. No. 564 352) for also inserting smaller GN formats (e.g. GN 1/9, GN 1/6, etc.)
* Eutectic plate -3°C, synthetic (Art. No. 569315)
* Menu cards incl. accessories (according to the full price list)

**Technical data**

Material: Polypropylene (PP)

Temperature

resistance: -25°C to +100°C

Insulating material: PUR foam, CFC-free

Capacity: e.g. 4x GN 1/1-55 or its subdivision

Weight 5,81kg

### Special features

* Maximum flexibility in loading with GN containers (max.4x GN 1/1-55 or their subdivision)
* GN containers can be inserted, which results in the option of stacking one on top of another
* Removal tools for easy stacking and removal of GN containers
* Dishwasher-safe up to a maximum of +96°C
* recyclable
* Moulded handles and skids

**Make**

Manufacturer: B.PRO

Model: BPT 320 ECO-C

 B.PROTHERM

Order No. 573 956