# Top-mounted frame GDD

**Dimensions**

Length: 963 mm

Width: 496 mm

Height: 231 mm

**Model**

The top-mounted frame GDD enables the correct storage, drying, transport and provision of Gastronorm lids with form-fitting seal. It is made completely of stainless steel, AISI 304. The top-mounted frame consists of an edged platform and welded round tube bars. Gastronorm lids in the GN 1/1, GN 1/2, GN 1/3 and GN 2/3 formats can be inserted between the individual bars. Thanks to the special design of the edging, the frame is ideal for mounting on a 10x6 serving trolley shelf.

**Accessories/options**

# Serving trolley SW 10x6-3 BASIC GDD (Order No. 574 166)

**Technical data**

Material: Stainless steel,

AISI 304

Weight: 10,2 kg

Loading bars: 31 pcs.

Bar material thickness: 5 mm

Capacity: 30x lids GDD 1/1 GN

or

60x lids GDD 1/2 GN

or

90x lids GDD 1/3 GN

### Special features

* Suitable for 10x6 serving trolley shelf

**Make**

Manufacturer: B.PRO

Type: Top-mounted frame  
GDD

Order No. 574167