**B.PRO COOK induction hob**

**with two round cooking zones**

**BC IH 2Z 5000**

**Dimensions:**

Length: 620 mm

Width: 400 mm

Height: 240 mm

**Housing design:**

The two-zone induction hob is made completely of micro-polished stainless steel (AISI 304), equipped with height-adjustable rotating feet. A 6 mm-thick glass ceramic surface is integrated flush in the cover and grouted with high-temperature resistant, highly elastic sealing compound. The glass ceramic surface is provided with two circular markings for the correct positioning of pots and pans. The air intake opening is below the unit and is via a removable air filter. The extracted air is removed via ventilation slits on the back of the top surface. The unit is designed to ensure that it can be positioned against a directly adjacent rear wall.

An operating area, angled towards the rear for improved viewing and operator ergonomics, is seamlessly installed on the front panel to hold the output regulator.

**Electrical equipment:**

The unit is equipped with a microprocessor-controlled E.G.O. induction generator. The cooking zones can be controlled independently of each other and are characterised by markings on the operating panel. Diameter per induction coil: 220 mm. Automatic pot detection from a pot/pan diameter of 120 mm. Continuous power control is carried out with two integrated rotary knobs installed in the operating area. An indicator light provides information on the operating mode and the error code in the event of faults. The unit is completely electrically wired and equipped with a 1.5 m connection cable with a 400 V, 16 A CEE plug which exits at a downward angle on the underside.

**Accessories/options:**

* Glass-ceramic cleaning scraper

Order No.: 568 489

* Clamping bar for bridging the gap to other B.PRO COOK units

Order No.: 574 298

**Technical data:**

Material: Stainles steel (AISI 304)

Glass-ceramic

Weight: approx. 27 kg

Protection type: IP X4

Heat emission sensitive: 0.35 kW

Heat emission latent: 0.14 kW

Cooking zones: 2 pieces, 220 mm dia.

Generator model: E.G.O.- QUAD Plus Duo Tray

Connected load: 400 V / 3N PE AC

50-60 Hz / 2 x 2.5 kW

(5 kW)

**Special features:**

* High efficiency through induction technology
* Low heat dissipation
* Energy-saving cooking
* Micro-polished surface made of stainless steel
* Angled operating area
* High-performance induction generator  
  made by E.G.O.

**Make:**

Manufacturer: B.PRO

Type: BC IH 2Z 5000

Order No.: 574 199