**B.PRO COOK griddles / Teppanyaki**

**with a flat griddle surface**

**BC GF 4200**

**Dimensions:**

Length: 620 mm

Width: 400 mm

Height: 240 mm

**Housing design:**

The griddle is made completely of micro-polished stainless steel (AISI 304), equipped with height-adjustable rotating feet. On the top surface, there is a recessed, flat, straight griddle surface (506 mm x 304 mm) made of tempered, corrosion-resistant chrome steel (1.2316), which is seamlessly welded all round. Large corner radii ensure optimal cleaning and hygiene. The griddle is 15 mm thick and guarantees optimal temperature storage and even heat distribution. In the front operating area of the griddle surface, there is an unheated resting zone (70 mm x 304 mm) with a round drain opening. On the body under the drain opening, there is a large, completely removable grease catch tray which can be detached at the front of the unit. An operating area, angled towards the rear for improved viewing and operator ergonomics, is seamlessly installed on the front panel to hold the temperature control. The unit is designed to ensure that it can be positioned against a directly adjacent rear wall.

**Electrical equipment:**

The unit is equipped with continuous temperature control. The even, full-surface heating of the griddle surface is made through tubular heating elements on the underside of the griddle. The surface temperature sensor quickly registers and compensates any temperature deviations from the setpoint. The temperature control from 80 °C bis 250 °C is carried out with a rotary knob installed in the operating area. 2 indicator lights provide information on the operating mode and heating phase. The unit is completely electrically wired and equipped with a 1.5 m connection cable with a 400 V, 16 A CEE plug which exits at a downward angle on the underside.

**Accessories/options:**

* Splash guard

Order No.: 574 256

* Griddle cleaning scraper

Order No.: 573 252

* Clamping bar for bridging the gap to other B.PRO COOK units

Order No.: 574 298

* B.PRO COOK non-stick care 500ml
maintains and protects the griddle surface and provides improved non-stick performance

Order No. 574 302

**Technical data:**

Material: Stainles steel (AISI 304)

Weight: approx. 34 kg

Grease catch tray: Capacity
approx. 1.6 litres

Trough depth: 30 mm

Protection type: IP X4

Heat emission sensitive: 1.39 kW

Heat emission latent: 1.68 kW

Connected load: 400 V / 3N PE AC

50-60 Hz / 4.2 kW

**Special features:**

* Griddle surface made of special steel
* Extremely powerful up to 250 °C
* Large-capacity grease catch tray
* Micro-polished surface made of stainless steel
* Angled operating area
* Scope of delivery incl. grease drain plug made of Teflon

**Make:**

Manufacturer: B.PRO

Type: BC GF 4200

Order No.: 574 204