**B.PRO COOK pasta cooker**

**BC PC 4800**

**Dimensions:**

Length: 620 mm

Width: 400 mm

Height: 240 mm

**Housing design:**

The pasta cooker is made completely of micro-polished stainless steel (AISI 304), equipped with height-adjustable rotating feet. The seamlessly deep-drawn basin with large corner radii in 1/1 GN format is made of corrosion-resistant V4A steel (1.4404). Capacity: approx. 20 litres. On the front of the basin, there is a round drain opening. The drain opening is covered with a lockable safety drain valve.

An operating area, angled towards the rear for improved viewing and operator ergonomics, is seamlessly installed on the front panel to hold the temperature control.

The unit is designed to ensure that it can be positioned against a directly adjacent rear wall.

**Electrical equipment:**

The bottom of the basin is heated using a special heating element on the underside, which guarantees very short heat-up times. The surface temperature sensor quickly registers and compensates any temperature deviations from the setpoint. Continuous temperature adjustment is carried out with an integrated rotary knob installed in the operating area. 2 indicator lights provide information on the operating mode and heating phase. The unit is completely electrically wired and equipped with a 1.5 m connection cable with a 400 V, 16 A CEE plug which exits at a downward angle on the underside.

**Accessories/options:**

* Pasta basket set of 6 baskets (approx. GN 1/6-100), each with insulated handles and an insertion frame

Order No.: 574 254

* Pasta basket set of 2 baskets (approx. GN 1/3-100) and 2 baskets (approx. GN 1/6-100), each with insulated handles and an insertion frame

Order No.: 574 255

* Gastronorm G-KEN G 1/1-95 cooking insert

Order No.: 550 971

* Lid with handle, GD 1/1

Order No.: 550 658

* Clamping bar for bridging the gap to other B.PRO COOK units

Order No.: 574 298

**Technical data:**

Material: Stainles steel (AISI 304)

Weight: approx. 14 kg

Protection type: IP X4

Heat emission sensitive: 0.60 kW

Heat emission latent: 0.96 kW

Connected load: 400 V / 3N PE AC

 50-60 Hz / 4.8 kW

**Special features:**

* Basin made of V4A steel (1.4404)
* Deep basin for GN 1/1-150
* Micro-polished surface made of stainless steel
* Angled operating area

**Make:**

Manufacturer: B.PRO

Type: BC PC 4800

Order No.: 574 210