**B.PRO COOK deep fryer**

**BC DF 5000**

**Dimensions:**

Length: 620 mm

Width: 400 mm

Height: 240 mm

Height incl. basket holder: 307 mm

**Housing design:**

The deep fryer is made completely of micro-polished stainless steel (AISI 304), equipped with height-adjustable rotating feet. The frying basin is seamlessly deep-drawn with large corner radii. Capacity: min. 5 litres, max. 6.5 litres. On the top surface, there is an attachment with a hanger for the deep-frying baskets. Using the handle secured to the attachment, the heating elements can be swivelled out for easy cleaning. On the front of the basin, there is a round drain opening. The drain opening is covered with a lockable safety drain valve.

An operating area, angled towards the rear for improved viewing and operator ergonomics, is seamlessly installed on the front panel to hold the temperature control.

The unit is designed to ensure that it can be positioned against a directly adjacent rear wall.

**Electrical equipment:**

Heating is provided through interior tubular heating elements, which guarantee very short heat-up times. There is a cold zone in the lower basin area. The frying basin temperature sensor quickly registers and compensates any temperature deviations from the setpoint. The temperature control from 100 °C bis 180 °C is carried out with a rotary knob installed in the operating area. 2 indicator lights provide information on the operating mode and heating phase. The unit is completely electrically wired and equipped with a 1.5 m connection cable with a 400 V, 16 A CEE plug which exits at a downward angle on the underside.

**Accessories/options:**

* Deep-frying basket set (2 pcs.), with insulated handles

Order No.: 574 258

* Deep-frying basket with insulated handle

Order No.: 574 259

* Clamping bar for bridging the gap to other B.PRO COOK units

Order No.: 574 298

**Technical data:**

Material: Stainles steel (AISI 304)

Weight: approx. 16 kg

Protection type: IP X4

Heat emission sensitive: 0.45 kW

Heat emission latent: 3.50 kW

Connected load: 400 V / 3N PE AC

 50-60 Hz / 5.0 kW

**Special features:**

* Swivelling heating element
* Unheated cold zone on the bottom of the basin
* Interior heating for short heat-up times
* Incl. lid to cover the frying basin
* Micro-polished surface made of stainless steel
* Angled operating area

**Make:**

Manufacturer: B.PRO

Type: BC DF 5000

Order No.: 574 211