**Tray clearing trolley, TAW 12 KN**

**Dimensions**

Length: 487 mm

Width: 607 mm

Height: 1550 mm

Height incl. trolley top (optional): 1586 mm

**Model**

The tray clearing trolley is one piece and is made completely of stainless steel, AISI 304. The frame construction is made of sturdy square tube (25x25 mm and 40x20 mm) and is welded all round.

The tray supports are made of round material with a dia. of 6 mm, and can be mounted and securely fastened within the frame construction. This means that the support frames can be completely removed if necessary. Through the bars that are welded at an angle, the tray supports are equipped with integrated push-through protection on both sides.

The tray clearing trolley can be loaded from both sides and has a capacity of 12 KN trays (460x344 mm). The support spacing is 100 mm.

The trolley is mobile on corrosion-resistant synthetic castors pursuant to DIN 18867, Part 8 (4 steering castors, 2 of which have brakes, castor diameter 125 mm). Synthetic (polyamide) round wall guards at all four corners protect against damage.

**Accessories/options**

* Thin sheet panelling on 2 sides, electrolytically galvanised double-sided, powder-coated in various colours, for mounting on the tray clearing trolley. Can be easily removed without any tools for cleaning.
* Stainless-steel panelling on 2 sides, for mounting on the tray clearing trolley. Can be easily removed without any tools for cleaning.
* Thin sheet panelling on 3 sides, electrolytically galvanised double-sided, powder-coated in various colours, for mounting on the tray clearing trolley. Can be easily removed without any tools for cleaning.
* Stainless-steel panelling on 3 sides, for mounting on the tray clearing trolley. Can be easily removed without any tools for cleaning.
* Door made of thin sheet, two-walled for more stability, electrolytically galvanised double-sided, powder-coated in various colours. Optionally available closed or with glass insert made of tempered safety glass.
* Door made of stainless steel. Optionally available closed or with glass insert made of tempered safety glass.
* Stainless-steel trolley top with all-round railing. For mounting on the tray clearing trolley. Can be easily removed without any tools for cleaning. The maximum permissible surface load is 20 kg.
* Base made of stainless steel for inserting in the frame construction. Can be easily removed without any tools for cleaning.
* Additional stainless-steel push-through protection
* Push handle short side
* Galvanised steel castor set

**Technical data**

Material: Stainless steel,
synthetic (polyamide)

Weight: approx. 21 kg

Max. load-bearing capacity
trolley: 150 kg

Max. load-bearing capacity/
support pair: 4.5 kg

Number of support pairs: 12

Capacity: 12 standard canteen trays,
 460x344 mm

Support spacing: 100 mm

Tray insertion: Lengthwise

### Special features

* Tray supports with integrated push-through protection on both sides
* Tray support frames are completely removable
* Optional panelling (on 2 or 3 sides) for mounting on the TAW. Can therefore be easily removed for cleaning.
* Attachments like panelling, doors, top and base can be retrofitted at any time.

**Make**

Manufacturer: B.PRO

Model: TAW 12 KN

Order No. 574327