# CE 88/ 61 – platform dispenser

**Dimensions**

Length: 1115 mm

Width: 730 mm

Height: 911 mm

Operating height: 900 mm

**Description**

**Structure**

The platform dispenser is made entirely of CNS 18/10 (AISI 304) with a specially ground matte surface finish (“microlised” surface).

The platform can be used for various types of crockery. The dispenser has a single-walled body in a closed and compact design.

Its interior panelling is entirely powder-coated to prevent the crockery from slipping and getting damaged.

The platform is supported by tension springs. By hanging or unhanging individual springs, the serving height can be adjusted according to the weight of the objects stacked.

A CNS safety push-pull handle with side bumper elements of plastic (polyamide) is mounted at the operator side.

The dispenser is made mobile by corrosion-resistant synthetic castors (4 steering castors, 2 of which have brakes, 125 mm dia.).

Very robust synthetic corner guards (polyamide) at all four corners protect the dispenser from being damaged.

### Accessories / options

* for other castor variations, please refer to our general price list

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 77 kg

Capacity: depends on type of crockery

Interior dims.: 881 x 611 mm

Emissions: The workplace-specific noise level of the unit is less than 70 dB(A)

### Special features

* protected against splash and jet water (IPX 5)
* entirely powder-coated interior panelling
* adjustable spring tension
* complies with DIN 18665, Part 6

**Make**

Manufacturer: B.PRO

Model: CE 88/ 61

Order No.: 574 892